/* 
 * This file is used to set the MAC address in NVRAM.
 * The MAC address of the Wi-Fi device may be configured in OTP and/or in NVRAM. 
 * If both OTP and NVRAM contains the MAC address then OTP programmed MAC address will be used. 
 * PSOC boards are usually programmed with OTP MAC address. 
 * MAC address is printed during WHD power up
 */

#define NVRAM_GENERATED_MAC_ADDRESS        "macaddr=00:A0:50:3c:c0:1d"
