#MicroXplorer Configuration settings - do not modify
ADC1.Channel-0\#ChannelRegularConversion=ADC_CHANNEL_0
ADC1.IPParameters=Rank-0\#ChannelRegularConversion,Channel-0\#ChannelRegularConversion,SamplingTime-0\#ChannelRegularConversion,OffsetNumber-0\#ChannelRegularConversion,OffsetSignedSaturation-0\#ChannelRegularConversion,NbrOfConversionFlag,master,Resolution,NbrOfConversion
ADC1.NbrOfConversion=1
ADC1.NbrOfConversionFlag=1
ADC1.OffsetNumber-0\#ChannelRegularConversion=ADC_OFFSET_NONE
ADC1.OffsetSignedSaturation-0\#ChannelRegularConversion=DISABLE
ADC1.Rank-0\#ChannelRegularConversion=1
ADC1.Resolution=ADC_RESOLUTION_16B
ADC1.SamplingTime-0\#ChannelRegularConversion=ADC_SAMPLETIME_1CYCLE_5
ADC1.master=1
ADC3.Channel-0\#ChannelRegularConversion=ADC_CHANNEL_0
ADC3.IPParameters=Rank-0\#ChannelRegularConversion,Channel-0\#ChannelRegularConversion,SamplingTime-0\#ChannelRegularConversion,OffsetNumber-0\#ChannelRegularConversion,OffsetSignedSaturation-0\#ChannelRegularConversion,NbrOfConversionFlag,NbrOfConversion
ADC3.NbrOfConversion=1
ADC3.NbrOfConversionFlag=1
ADC3.OffsetNumber-0\#ChannelRegularConversion=ADC_OFFSET_NONE
ADC3.OffsetSignedSaturation-0\#ChannelRegularConversion=DISABLE
ADC3.Rank-0\#ChannelRegularConversion=1
ADC3.SamplingTime-0\#ChannelRegularConversion=ADC_SAMPLETIME_1CYCLE_5
CAD.formats=
CAD.pinconfig=
CAD.provider=
CORTEX_M7.AccessPermission_S-Cortex_Memory_Protection_Unit_Region1_Settings_S=MPU_REGION_FULL_ACCESS
CORTEX_M7.AccessPermission_S-Cortex_Memory_Protection_Unit_Region2_Settings_S=MPU_REGION_FULL_ACCESS
CORTEX_M7.AccessPermission_S-Cortex_Memory_Protection_Unit_Region3_Settings_S=MPU_REGION_FULL_ACCESS
CORTEX_M7.AccessPermission_S-Cortex_Memory_Protection_Unit_Region4_Settings_S=MPU_REGION_FULL_ACCESS
CORTEX_M7.BaseAddress_S-Cortex_Memory_Protection_Unit_Region1_Settings_S=0x30000000
CORTEX_M7.BaseAddress_S-Cortex_Memory_Protection_Unit_Region2_Settings_S=0x30020000
CORTEX_M7.BaseAddress_S-Cortex_Memory_Protection_Unit_Region3_Settings_S=0xC0000000
CORTEX_M7.BaseAddress_S-Cortex_Memory_Protection_Unit_Region4_Settings_S=0x90000000
CORTEX_M7.CPU_DCache=Enabled
CORTEX_M7.CPU_ICache=Enabled
CORTEX_M7.DisableExec_S-Cortex_Memory_Protection_Unit_Region1_Settings_S=MPU_INSTRUCTION_ACCESS_DISABLE
CORTEX_M7.DisableExec_S-Cortex_Memory_Protection_Unit_Region2_Settings_S=MPU_INSTRUCTION_ACCESS_DISABLE
CORTEX_M7.DisableExec_S-Cortex_Memory_Protection_Unit_Region3_Settings_S=MPU_INSTRUCTION_ACCESS_DISABLE
CORTEX_M7.DisableExec_S-Cortex_Memory_Protection_Unit_Region4_Settings_S=MPU_INSTRUCTION_ACCESS_DISABLE
CORTEX_M7.Enable_S-Cortex_Memory_Protection_Unit_Region1_Settings_S=MPU_REGION_ENABLE
CORTEX_M7.Enable_S-Cortex_Memory_Protection_Unit_Region2_Settings_S=MPU_REGION_ENABLE
CORTEX_M7.Enable_S-Cortex_Memory_Protection_Unit_Region3_Settings_S=MPU_REGION_ENABLE
CORTEX_M7.Enable_S-Cortex_Memory_Protection_Unit_Region4_Settings_S=MPU_REGION_ENABLE
CORTEX_M7.IPParameters=default_mode_Activation,CPU_ICache,CPU_DCache,Enable_S-Cortex_Memory_Protection_Unit_Region1_Settings_S,BaseAddress_S-Cortex_Memory_Protection_Unit_Region1_Settings_S,Size_S-Cortex_Memory_Protection_Unit_Region1_Settings_S,AccessPermission_S-Cortex_Memory_Protection_Unit_Region1_Settings_S,DisableExec_S-Cortex_Memory_Protection_Unit_Region1_Settings_S,IsShareable_S-Cortex_Memory_Protection_Unit_Region1_Settings_S,IsCacheable_S-Cortex_Memory_Protection_Unit_Region1_Settings_S,IsBufferable_S-Cortex_Memory_Protection_Unit_Region1_Settings_S,Enable_S-Cortex_Memory_Protection_Unit_Region3_Settings_S,BaseAddress_S-Cortex_Memory_Protection_Unit_Region3_Settings_S,Size_S-Cortex_Memory_Protection_Unit_Region3_Settings_S,AccessPermission_S-Cortex_Memory_Protection_Unit_Region3_Settings_S,DisableExec_S-Cortex_Memory_Protection_Unit_Region3_Settings_S,IsShareable_S-Cortex_Memory_Protection_Unit_Region3_Settings_S,IsCacheable_S-Cortex_Memory_Protection_Unit_Region3_Settings_S,IsBufferable_S-Cortex_Memory_Protection_Unit_Region3_Settings_S,TypeExtField_S-Cortex_Memory_Protection_Unit_Region1_Settings_S,Enable_S-Cortex_Memory_Protection_Unit_Region2_Settings_S,BaseAddress_S-Cortex_Memory_Protection_Unit_Region2_Settings_S,Size_S-Cortex_Memory_Protection_Unit_Region2_Settings_S,AccessPermission_S-Cortex_Memory_Protection_Unit_Region2_Settings_S,DisableExec_S-Cortex_Memory_Protection_Unit_Region2_Settings_S,IsShareable_S-Cortex_Memory_Protection_Unit_Region2_Settings_S,IsBufferable_S-Cortex_Memory_Protection_Unit_Region2_Settings_S,Enable_S-Cortex_Memory_Protection_Unit_Region4_Settings_S,BaseAddress_S-Cortex_Memory_Protection_Unit_Region4_Settings_S,Size_S-Cortex_Memory_Protection_Unit_Region4_Settings_S,AccessPermission_S-Cortex_Memory_Protection_Unit_Region4_Settings_S,DisableExec_S-Cortex_Memory_Protection_Unit_Region4_Settings_S,IsShareable_S-Cortex_Memory_Protection_Unit_Region4_Settings_S,IsCacheable_S-Cortex_Memory_Protection_Unit_Region4_Settings_S,IsBufferable_S-Cortex_Memory_Protection_Unit_Region4_Settings_S
CORTEX_M7.IsBufferable_S-Cortex_Memory_Protection_Unit_Region1_Settings_S=MPU_ACCESS_NOT_BUFFERABLE
CORTEX_M7.IsBufferable_S-Cortex_Memory_Protection_Unit_Region2_Settings_S=MPU_ACCESS_BUFFERABLE
CORTEX_M7.IsBufferable_S-Cortex_Memory_Protection_Unit_Region3_Settings_S=MPU_ACCESS_BUFFERABLE
CORTEX_M7.IsBufferable_S-Cortex_Memory_Protection_Unit_Region4_Settings_S=MPU_ACCESS_BUFFERABLE
CORTEX_M7.IsCacheable_S-Cortex_Memory_Protection_Unit_Region1_Settings_S=MPU_ACCESS_NOT_CACHEABLE
CORTEX_M7.IsCacheable_S-Cortex_Memory_Protection_Unit_Region3_Settings_S=MPU_ACCESS_CACHEABLE
CORTEX_M7.IsCacheable_S-Cortex_Memory_Protection_Unit_Region4_Settings_S=MPU_ACCESS_CACHEABLE
CORTEX_M7.IsShareable_S-Cortex_Memory_Protection_Unit_Region1_Settings_S=MPU_ACCESS_SHAREABLE
CORTEX_M7.IsShareable_S-Cortex_Memory_Protection_Unit_Region2_Settings_S=MPU_ACCESS_SHAREABLE
CORTEX_M7.IsShareable_S-Cortex_Memory_Protection_Unit_Region3_Settings_S=MPU_ACCESS_SHAREABLE
CORTEX_M7.IsShareable_S-Cortex_Memory_Protection_Unit_Region4_Settings_S=MPU_ACCESS_SHAREABLE
CORTEX_M7.Size_S-Cortex_Memory_Protection_Unit_Region1_Settings_S=MPU_REGION_SIZE_128KB
CORTEX_M7.Size_S-Cortex_Memory_Protection_Unit_Region2_Settings_S=MPU_REGION_SIZE_4KB
CORTEX_M7.Size_S-Cortex_Memory_Protection_Unit_Region3_Settings_S=MPU_REGION_SIZE_32MB
CORTEX_M7.Size_S-Cortex_Memory_Protection_Unit_Region4_Settings_S=MPU_REGION_SIZE_32MB
CORTEX_M7.TypeExtField_S-Cortex_Memory_Protection_Unit_Region1_Settings_S=MPU_TEX_LEVEL1
CORTEX_M7.default_mode_Activation=1
CortexM4.IPs=BDMA,CORTEX_M4\:I,DMA,FATFS_M4\:I,FREERTOS_M4\:I,GPIO,IWDG2\:I,MDMA,NVIC2\:I,OPENAMP_M4\:I,PDM2PCM_M4\:I,PWR,RCC,RESMGR_UTILITY,SYS_M4\:I,USB_DEVICE_M4\:I,USB_HOST_M4\:I,VREFBUF,WWDG2\:I
CortexM7.IPs=BDMA\:I,CORTEX_M7\:I,DMA\:I,FATFS_M7\:I,FREERTOS_M7\:I,GPIO\:I,IWDG1\:I,MDMA\:I,NVIC1\:I,OPENAMP_M7\:I,PDM2PCM_M7\:I,PWR\:I,RCC\:I,RESMGR_UTILITY\:I,SYS\:I,USB_DEVICE_M7\:I,USB_HOST_M7\:I,VREFBUF\:I,WWDG1\:I,MEMORYMAP\:I,TIM15\:I,USART1\:I,LTDC\:I,DSIHOST\:I,FMC\:I,DMA2D\:I,I2C3\:I,ETH\:I,LWIP\:I,USB_OTG_HS\:I,USB_OTG_FS\:I,DCMI\:I,QUADSPI\:I,USART6\:I,FDCAN1\:I,I2C1\:I,I2S2\:I,USART2\:I,LPTIM1\:I,SDMMC1\:I,ADC1\:I,ADC3\:I
CortexM7.Pins=PB5,PH15,PD7,PE5,PE3,PI9,PI8,PE6,PI10,PI11,PC7,PI14,PG3,PF6,PF7,PF8,PF9,PH2,PA0,PH3,PH4,PH5,PB10,PB11,PH11,PB2,PA5,PB1,PH6,PB0
DCMI.HSPolarity=DCMI_HSPOLARITY_HIGH
DCMI.IPParameters=JPEGMode,PCKPolarity,VSPolarity,HSPolarity
DCMI.JPEGMode=DCMI_JPEG_DISABLE
DCMI.PCKPolarity=DCMI_PCKPOLARITY_RISING
DCMI.VSPolarity=DCMI_VSPOLARITY_HIGH
DMA2D.ColorMode=DMA2D_OUTPUT_ARGB8888
DMA2D.IPParameters=ColorMode,Mode
DMA2D.Mode=DMA2D_R2M
DSIHOST.ClockLaneLP2HSTime=32
DSIHOST.DataLaneLP2HSTime=24
DSIHOST.HorizontalBackPorch=192
DSIHOST.HorizontalLine=1612
DSIHOST.HorizontalSyncActive=49
DSIHOST.IPParameters=NumberOfLanes,Mode,LPHorizontalFrontPorchEnable,LPHorizontalBackPorchEnable,LPVerticalActiveEnable,LPVerticalFrontPorchEnable,LPVerticalBackPorchEnable,LPVerticalSyncActiveEnable,TimingPHY_THS_ZERO_Enable,TimingPHY_THS_ZERO_Value,ClockLaneLP2HSTime,DataLaneLP2HSTime,HorizontalSyncActive,HorizontalBackPorch,HorizontalLine,LPCommandEnable,LPLargestPacketSize
DSIHOST.LPCommandEnable=DSI_LP_COMMAND_ENABLE
DSIHOST.LPHorizontalBackPorchEnable=DSI_LP_HBP_ENABLE
DSIHOST.LPHorizontalFrontPorchEnable=DSI_LP_HFP_ENABLE
DSIHOST.LPLargestPacketSize=23
DSIHOST.LPVerticalActiveEnable=DSI_LP_VACT_ENABLE
DSIHOST.LPVerticalBackPorchEnable=DSI_LP_VBP_ENABLE
DSIHOST.LPVerticalFrontPorchEnable=DSI_LP_VFP_ENABLE
DSIHOST.LPVerticalSyncActiveEnable=DSI_LP_VSYNC_ENABLE
DSIHOST.Mode=DSI_VID_MODE_BURST
DSIHOST.NumberOfLanes=DSI_TWO_DATA_LANES
DSIHOST.TimingPHY_THS_ZERO_Enable=ENABLE
DSIHOST.TimingPHY_THS_ZERO_Value=200
DSI_CKN.GPIOParameters=PinAttribute
DSI_CKN.Mode=DSIHost_Video
DSI_CKN.PinAttribute=CortexM7
DSI_CKN.Signal=DSIHOST_CKN
DSI_CKP.GPIOParameters=PinAttribute
DSI_CKP.Mode=DSIHost_Video
DSI_CKP.PinAttribute=CortexM7
DSI_CKP.Signal=DSIHOST_CKP
DSI_D0N.GPIOParameters=PinAttribute
DSI_D0N.Mode=DSIHost_Video
DSI_D0N.PinAttribute=CortexM7
DSI_D0N.Signal=DSIHOST_D0N
DSI_D0P.GPIOParameters=PinAttribute
DSI_D0P.Mode=DSIHost_Video
DSI_D0P.PinAttribute=CortexM7
DSI_D0P.Signal=DSIHOST_D0P
DSI_D1N.GPIOParameters=PinAttribute
DSI_D1N.Mode=DSIHost_Video
DSI_D1N.PinAttribute=CortexM7
DSI_D1N.Signal=DSIHOST_D1N
DSI_D1P.GPIOParameters=PinAttribute
DSI_D1P.Mode=DSIHost_Video
DSI_D1P.PinAttribute=CortexM7
DSI_D1P.Signal=DSIHOST_D1P
Dma.DCMI.0.Direction=DMA_PERIPH_TO_MEMORY
Dma.DCMI.0.EventEnable=DISABLE
Dma.DCMI.0.FIFOMode=DMA_FIFOMODE_ENABLE
Dma.DCMI.0.FIFOThreshold=DMA_FIFO_THRESHOLD_FULL
Dma.DCMI.0.Instance=DMA1_Stream2
Dma.DCMI.0.MemBurst=DMA_MBURST_SINGLE
Dma.DCMI.0.MemDataAlignment=DMA_MDATAALIGN_WORD
Dma.DCMI.0.MemInc=DMA_MINC_ENABLE
Dma.DCMI.0.Mode=DMA_NORMAL
Dma.DCMI.0.PeriphBurst=DMA_PBURST_SINGLE
Dma.DCMI.0.PeriphDataAlignment=DMA_PDATAALIGN_WORD
Dma.DCMI.0.PeriphInc=DMA_PINC_DISABLE
Dma.DCMI.0.Polarity=HAL_DMAMUX_REQ_GEN_RISING
Dma.DCMI.0.Priority=DMA_PRIORITY_LOW
Dma.DCMI.0.RequestNumber=1
Dma.DCMI.0.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority,FIFOMode,FIFOThreshold,MemBurst,PeriphBurst,SignalID,Polarity,RequestNumber,SyncSignalID,SyncPolarity,SyncEnable,EventEnable,SyncRequestNumber
Dma.DCMI.0.SignalID=NONE
Dma.DCMI.0.SyncEnable=DISABLE
Dma.DCMI.0.SyncPolarity=HAL_DMAMUX_SYNC_NO_EVENT
Dma.DCMI.0.SyncRequestNumber=1
Dma.DCMI.0.SyncSignalID=NONE
Dma.Request0=DCMI
Dma.Request1=SPI2_RX
Dma.Request2=SPI2_TX
Dma.Request3=USART2_RX
Dma.Request4=USART2_TX
Dma.RequestsNb=5
Dma.SPI2_RX.1.Direction=DMA_PERIPH_TO_MEMORY
Dma.SPI2_RX.1.EventEnable=DISABLE
Dma.SPI2_RX.1.FIFOMode=DMA_FIFOMODE_ENABLE
Dma.SPI2_RX.1.FIFOThreshold=DMA_FIFO_THRESHOLD_FULL
Dma.SPI2_RX.1.Instance=DMA1_Stream0
Dma.SPI2_RX.1.MemBurst=DMA_MBURST_SINGLE
Dma.SPI2_RX.1.MemDataAlignment=DMA_MDATAALIGN_HALFWORD
Dma.SPI2_RX.1.MemInc=DMA_MINC_ENABLE
Dma.SPI2_RX.1.Mode=DMA_NORMAL
Dma.SPI2_RX.1.PeriphBurst=DMA_PBURST_SINGLE
Dma.SPI2_RX.1.PeriphDataAlignment=DMA_PDATAALIGN_HALFWORD
Dma.SPI2_RX.1.PeriphInc=DMA_PINC_DISABLE
Dma.SPI2_RX.1.Polarity=HAL_DMAMUX_REQ_GEN_RISING
Dma.SPI2_RX.1.Priority=DMA_PRIORITY_LOW
Dma.SPI2_RX.1.RequestNumber=1
Dma.SPI2_RX.1.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority,FIFOMode,FIFOThreshold,MemBurst,PeriphBurst,SignalID,Polarity,RequestNumber,SyncSignalID,SyncPolarity,SyncEnable,EventEnable,SyncRequestNumber
Dma.SPI2_RX.1.SignalID=NONE
Dma.SPI2_RX.1.SyncEnable=DISABLE
Dma.SPI2_RX.1.SyncPolarity=HAL_DMAMUX_SYNC_NO_EVENT
Dma.SPI2_RX.1.SyncRequestNumber=1
Dma.SPI2_RX.1.SyncSignalID=NONE
Dma.SPI2_TX.2.Direction=DMA_MEMORY_TO_PERIPH
Dma.SPI2_TX.2.EventEnable=DISABLE
Dma.SPI2_TX.2.FIFOMode=DMA_FIFOMODE_ENABLE
Dma.SPI2_TX.2.FIFOThreshold=DMA_FIFO_THRESHOLD_FULL
Dma.SPI2_TX.2.Instance=DMA1_Stream1
Dma.SPI2_TX.2.MemBurst=DMA_MBURST_SINGLE
Dma.SPI2_TX.2.MemDataAlignment=DMA_MDATAALIGN_HALFWORD
Dma.SPI2_TX.2.MemInc=DMA_MINC_ENABLE
Dma.SPI2_TX.2.Mode=DMA_NORMAL
Dma.SPI2_TX.2.PeriphBurst=DMA_PBURST_SINGLE
Dma.SPI2_TX.2.PeriphDataAlignment=DMA_PDATAALIGN_HALFWORD
Dma.SPI2_TX.2.PeriphInc=DMA_PINC_DISABLE
Dma.SPI2_TX.2.Polarity=HAL_DMAMUX_REQ_GEN_RISING
Dma.SPI2_TX.2.Priority=DMA_PRIORITY_LOW
Dma.SPI2_TX.2.RequestNumber=1
Dma.SPI2_TX.2.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority,FIFOMode,FIFOThreshold,MemBurst,PeriphBurst,SignalID,Polarity,RequestNumber,SyncSignalID,SyncPolarity,SyncEnable,EventEnable,SyncRequestNumber
Dma.SPI2_TX.2.SignalID=NONE
Dma.SPI2_TX.2.SyncEnable=DISABLE
Dma.SPI2_TX.2.SyncPolarity=HAL_DMAMUX_SYNC_NO_EVENT
Dma.SPI2_TX.2.SyncRequestNumber=1
Dma.SPI2_TX.2.SyncSignalID=NONE
Dma.USART2_RX.3.Direction=DMA_PERIPH_TO_MEMORY
Dma.USART2_RX.3.EventEnable=DISABLE
Dma.USART2_RX.3.FIFOMode=DMA_FIFOMODE_DISABLE
Dma.USART2_RX.3.Instance=DMA1_Stream3
Dma.USART2_RX.3.MemDataAlignment=DMA_MDATAALIGN_BYTE
Dma.USART2_RX.3.MemInc=DMA_MINC_ENABLE
Dma.USART2_RX.3.Mode=DMA_NORMAL
Dma.USART2_RX.3.PeriphDataAlignment=DMA_PDATAALIGN_BYTE
Dma.USART2_RX.3.PeriphInc=DMA_PINC_DISABLE
Dma.USART2_RX.3.Polarity=HAL_DMAMUX_REQ_GEN_RISING
Dma.USART2_RX.3.Priority=DMA_PRIORITY_LOW
Dma.USART2_RX.3.RequestNumber=1
Dma.USART2_RX.3.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority,FIFOMode,SignalID,Polarity,RequestNumber,SyncSignalID,SyncPolarity,SyncEnable,EventEnable,SyncRequestNumber
Dma.USART2_RX.3.SignalID=NONE
Dma.USART2_RX.3.SyncEnable=DISABLE
Dma.USART2_RX.3.SyncPolarity=HAL_DMAMUX_SYNC_NO_EVENT
Dma.USART2_RX.3.SyncRequestNumber=1
Dma.USART2_RX.3.SyncSignalID=NONE
Dma.USART2_TX.4.Direction=DMA_MEMORY_TO_PERIPH
Dma.USART2_TX.4.EventEnable=DISABLE
Dma.USART2_TX.4.FIFOMode=DMA_FIFOMODE_DISABLE
Dma.USART2_TX.4.Instance=DMA1_Stream4
Dma.USART2_TX.4.MemDataAlignment=DMA_MDATAALIGN_BYTE
Dma.USART2_TX.4.MemInc=DMA_MINC_ENABLE
Dma.USART2_TX.4.Mode=DMA_NORMAL
Dma.USART2_TX.4.PeriphDataAlignment=DMA_PDATAALIGN_BYTE
Dma.USART2_TX.4.PeriphInc=DMA_PINC_DISABLE
Dma.USART2_TX.4.Polarity=HAL_DMAMUX_REQ_GEN_RISING
Dma.USART2_TX.4.Priority=DMA_PRIORITY_LOW
Dma.USART2_TX.4.RequestNumber=1
Dma.USART2_TX.4.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority,FIFOMode,SignalID,Polarity,RequestNumber,SyncSignalID,SyncPolarity,SyncEnable,EventEnable,SyncRequestNumber
Dma.USART2_TX.4.SignalID=NONE
Dma.USART2_TX.4.SyncEnable=DISABLE
Dma.USART2_TX.4.SyncPolarity=HAL_DMAMUX_SYNC_NO_EVENT
Dma.USART2_TX.4.SyncRequestNumber=1
Dma.USART2_TX.4.SyncSignalID=NONE
ETH.IPParameters=MediaInterface,RxDescAddress,TxDescAddress,RxBufferAddress
ETH.MediaInterface=HAL_ETH_RMII_MODE
ETH.RxBufferAddress=0x30020200
ETH.RxDescAddress=0x30020000
ETH.TxDescAddress=0x30020100
FATFS.BSP.number=1
FATFS0.BSP.STBoard=false
FATFS0.BSP.api=Unknown
FATFS0.BSP.component=
FATFS0.BSP.condition=
FATFS0.BSP.instance=PI14
FATFS0.BSP.ip=GPIO
FATFS0.BSP.mode=Input
FATFS0.BSP.name=Detect_SDIO
FATFS0.BSP.semaphore=
FATFS0.BSP.solution=PI14
FDCAN1.CalculateBaudRateNominal=125000
FDCAN1.CalculateTimeBitNominal=8000
FDCAN1.CalculateTimeQuantumNominal=25.0
FDCAN1.IPParameters=CalculateTimeQuantumNominal,CalculateTimeBitNominal,CalculateBaudRateNominal,RxFifo0ElmtsNbr,StdFiltersNbr,TxFifoQueueElmtsNbr,NominalPrescaler,NominalTimeSeg1,NominalTimeSeg2
FDCAN1.NominalPrescaler=2
FDCAN1.NominalTimeSeg1=239
FDCAN1.NominalTimeSeg2=80
FDCAN1.RxFifo0ElmtsNbr=1
FDCAN1.StdFiltersNbr=1
FDCAN1.TxFifoQueueElmtsNbr=1
FMC.CASLatency1=FMC_SDRAM_CAS_LATENCY_2
FMC.ColumnBitsNumber1=FMC_SDRAM_COLUMN_BITS_NUM_9
FMC.ExitSelfRefreshDelay1=7
FMC.IPParameters=ColumnBitsNumber1,CASLatency1,SDClockPeriod1,SDClockPeriod2,ReadBurst1,ReadBurst2,SelfRefreshTime1,RowCycleDelay1,RowCycleDelay2,WriteRecoveryTime1,RPDelay1,RPDelay2,LoadToActiveDelay1,ExitSelfRefreshDelay1,RCDDelay1
FMC.LoadToActiveDelay1=2
FMC.RCDDelay1=2
FMC.RPDelay1=2
FMC.RPDelay2=2
FMC.ReadBurst1=FMC_SDRAM_RBURST_ENABLE
FMC.ReadBurst2=FMC_SDRAM_RBURST_ENABLE
FMC.RowCycleDelay1=7
FMC.RowCycleDelay2=7
FMC.SDClockPeriod1=FMC_SDRAM_CLOCK_PERIOD_2
FMC.SDClockPeriod2=FMC_SDRAM_CLOCK_PERIOD_2
FMC.SelfRefreshTime1=4
FMC.WriteRecoveryTime1=3
FREERTOS_M7.FootprintOK=true
FREERTOS_M7.IPParameters=Tasks01,FootprintOK,configUSE_NEWLIB_REENTRANT,configTIMER_TASK_STACK_DEPTH,configMINIMAL_STACK_SIZE,configTOTAL_HEAP_SIZE
FREERTOS_M7.Tasks01=MainTask,24,512,mainTask,Default,NULL,Dynamic,NULL,NULL
FREERTOS_M7.configMINIMAL_STACK_SIZE=128
FREERTOS_M7.configTIMER_TASK_STACK_DEPTH=1024
FREERTOS_M7.configTOTAL_HEAP_SIZE=131072
FREERTOS_M7.configUSE_NEWLIB_REENTRANT=1
File.Version=6
GPIO.groupedBy=Group By Peripherals
I2C1.IPParameters=Timing
I2C1.Timing=0x10C0ECFF
I2C3.IPParameters=Timing
I2C3.Timing=0x10C0ECFF
I2S2.AudioFreq=I2S_AUDIOFREQ_48K
I2S2.ErrorAudioFreq=1.72 %
I2S2.IPParameters=Instance,RealAudioFreq,ErrorAudioFreq,AudioFreq
I2S2.Instance=SPI$Index
I2S2.RealAudioFreq=48.828 KHz
KeepUserPlacement=false
LTDC.ActiveH=600
LTDC.ActiveW=1024
LTDC.Alpha_L0=255
LTDC.BlendingFactor1_L0=LTDC_BLENDING_FACTOR1_PAxCA
LTDC.BlendingFactor2_L0=LTDC_BLENDING_FACTOR2_PAxCA
LTDC.FBStartAdress_L0=0xC0000000
LTDC.HBP=160
LTDC.HFP=160
LTDC.HSync=1
LTDC.IPParameters=Layers,WindowX1_L0,WindowY1_L0,BlendingFactor1_L0,BlendingFactor2_L0,FBStartAdress_L0,ImageWidth_L0,ImageHeight_L0,HSync,HBP,HFP,ActiveW,VSync,VBP,ActiveH,VFP,Alpha_L0,PixelFormat_L0
LTDC.ImageHeight_L0=600
LTDC.ImageWidth_L0=1024
LTDC.Layers=0
LTDC.PixelFormat_L0=LTDC_PIXEL_FORMAT_RGB565
LTDC.VBP=23
LTDC.VFP=12
LTDC.VSync=1
LTDC.WindowX1_L0=1024
LTDC.WindowY1_L0=600
LWIP.BSP.number=1
LWIP.DEFAULT_ACCEPTMBOX_SIZE=12
LWIP.DEFAULT_RAW_RECVMBOX_SIZE=12
LWIP.DEFAULT_TCP_RECVMBOX_SIZE=12
LWIP.DEFAULT_THREAD_STACKSIZE=2048
LWIP.IPParameters=TCP_MSS,TCP_SND_BUF,TCP_SND_QUEUELEN,LWIP_RAM_HEAP_POINTER,MEM_SIZE,DEFAULT_THREAD_STACKSIZE,TCPIP_THREAD_STACKSIZE,LWIP_RAW,DEFAULT_RAW_RECVMBOX_SIZE,DEFAULT_TCP_RECVMBOX_SIZE,DEFAULT_ACCEPTMBOX_SIZE,TCPIP_MBOX_SIZE,LWIP_SO_RCVTIMEO,LWIP_NETIF_API
LWIP.LWIP_NETIF_API=1
LWIP.LWIP_RAM_HEAP_POINTER=0xC0C00000
LWIP.LWIP_RAW=1
LWIP.LWIP_SO_RCVTIMEO=1
LWIP.MEM_SIZE=131048
LWIP.TCPIP_MBOX_SIZE=32
LWIP.TCPIP_THREAD_STACKSIZE=2048
LWIP.TCP_MSS=1460
LWIP.TCP_SND_BUF=5840
LWIP.TCP_SND_QUEUELEN=16
LWIP.Version=v2.1.2_Cube
LWIP0.BSP.STBoard=false
LWIP0.BSP.api=BSP_COMPONENT_DRIVER
LWIP0.BSP.component=LAN8742
LWIP0.BSP.condition=
LWIP0.BSP.instance=LAN8742
LWIP0.BSP.ip=
LWIP0.BSP.mode=
LWIP0.BSP.name=Driver_PHY
LWIP0.BSP.semaphore=S_LAN8742
LWIP0.BSP.solution=LAN8742
MMTAppReg1.MEMORYMAP.AppRegionName=RAM
MMTAppReg1.MEMORYMAP.ContextName=CortexM7
MMTAppReg1.MEMORYMAP.CoreName=ARM Cortex-M7
MMTAppReg1.MEMORYMAP.DefaultDataRegion=true
MMTAppReg1.MEMORYMAP.IPParameters=StartAddress,Size,CoreName,ContextName,Name,DefaultDataRegion
MMTAppReg1.MEMORYMAP.Name=RAM
MMTAppReg1.MEMORYMAP.Size=131072
MMTAppReg1.MEMORYMAP.StartAddress=0x20000000
MMTAppReg10.MEMORYMAP.AppRegionName=M4 non Shared Region
MMTAppReg10.MEMORYMAP.ContextLink=reserved
MMTAppReg10.MEMORYMAP.ContextName=CortexM7
MMTAppReg10.MEMORYMAP.CoreName=ARM Cortex-M7
MMTAppReg10.MEMORYMAP.IPParameters=StartAddress,Size,CoreName,MemType,ContextName,Name,ReservedRegion,ContextLink
MMTAppReg10.MEMORYMAP.MemType=ROM
MMTAppReg10.MEMORYMAP.Name=M4 non Shared Region
MMTAppReg10.MEMORYMAP.ReservedRegion=true
MMTAppReg10.MEMORYMAP.Size=1048576
MMTAppReg10.MEMORYMAP.StartAddress=0x08100000
MMTAppReg11.MEMORYMAP.AppRegionName=DISP_MEM
MMTAppReg11.MEMORYMAP.Cacheability=NonCacheable
MMTAppReg11.MEMORYMAP.ContextLink=shared
MMTAppReg11.MEMORYMAP.ContextName=CortexM7
MMTAppReg11.MEMORYMAP.CoreName=ARM Cortex-M7
MMTAppReg11.MEMORYMAP.IPParameters=StartAddress,Size,CoreName,SizeUnit,MemSource,ContextName,Name,XN,Cacheability,ContextLink,Shareability,InvalidRegion
MMTAppReg11.MEMORYMAP.InvalidRegion=true
MMTAppReg11.MEMORYMAP.MemSource=EXT
MMTAppReg11.MEMORYMAP.Name=DISP_MEM
MMTAppReg11.MEMORYMAP.Shareability=Shareable
MMTAppReg11.MEMORYMAP.Size=33554432
MMTAppReg11.MEMORYMAP.SizeUnit=MB
MMTAppReg11.MEMORYMAP.StartAddress=0xC0000000
MMTAppReg11.MEMORYMAP.XN=NotPermitted
MMTAppReg12.MEMORYMAP.AppRegionName=M7 non Shared Region
MMTAppReg12.MEMORYMAP.ContextLink=reserved
MMTAppReg12.MEMORYMAP.ContextName=CortexM4
MMTAppReg12.MEMORYMAP.CoreName=ARM Cortex-M4
MMTAppReg12.MEMORYMAP.IPParameters=StartAddress,Size,CoreName,MemSource,ContextName,Name,ReservedRegion,ContextLink,InvalidRegion
MMTAppReg12.MEMORYMAP.InvalidRegion=true
MMTAppReg12.MEMORYMAP.MemSource=EXT
MMTAppReg12.MEMORYMAP.Name=M7 non Shared Region
MMTAppReg12.MEMORYMAP.ReservedRegion=true
MMTAppReg12.MEMORYMAP.Size=33554432
MMTAppReg12.MEMORYMAP.StartAddress=0xc0000000
MMTAppReg13.MEMORYMAP.AppRegionName=RxDescriptor
MMTAppReg13.MEMORYMAP.ContextLink=shared
MMTAppReg13.MEMORYMAP.ContextName=CortexM7
MMTAppReg13.MEMORYMAP.CoreName=ARM Cortex-M7
MMTAppReg13.MEMORYMAP.IPParameters=StartAddress,Size,CoreName,SizeUnit,ContextName,Name,ContextLink,Shareability,Shared
MMTAppReg13.MEMORYMAP.Name=RxDescriptor
MMTAppReg13.MEMORYMAP.Shareability=Shareable
MMTAppReg13.MEMORYMAP.Shared=true
MMTAppReg13.MEMORYMAP.Size=128
MMTAppReg13.MEMORYMAP.SizeUnit=B
MMTAppReg13.MEMORYMAP.StartAddress=0x30020000
MMTAppReg14.MEMORYMAP.AppRegionName=RxDescriptor
MMTAppReg14.MEMORYMAP.ContextLink=reserved
MMTAppReg14.MEMORYMAP.ContextName=CortexM4
MMTAppReg14.MEMORYMAP.CoreName=ARM Cortex-M4
MMTAppReg14.MEMORYMAP.IPParameters=StartAddress,Size,CoreName,SizeUnit,ContextName,Name,ContextLink,Shared,Shareability
MMTAppReg14.MEMORYMAP.Name=RxDescriptor
MMTAppReg14.MEMORYMAP.Shareability=Shareable
MMTAppReg14.MEMORYMAP.Shared=true
MMTAppReg14.MEMORYMAP.Size=128
MMTAppReg14.MEMORYMAP.SizeUnit=B
MMTAppReg14.MEMORYMAP.StartAddress=0x30020000
MMTAppReg15.MEMORYMAP.AppRegionName=TxDescriptor
MMTAppReg15.MEMORYMAP.ContextLink=shared
MMTAppReg15.MEMORYMAP.ContextName=CortexM7
MMTAppReg15.MEMORYMAP.CoreName=ARM Cortex-M7
MMTAppReg15.MEMORYMAP.IPParameters=StartAddress,Size,CoreName,SizeUnit,ContextName,Name,ContextLink,Shareability,Shared
MMTAppReg15.MEMORYMAP.Name=TxDescriptor
MMTAppReg15.MEMORYMAP.Shareability=Shareable
MMTAppReg15.MEMORYMAP.Shared=true
MMTAppReg15.MEMORYMAP.Size=128
MMTAppReg15.MEMORYMAP.SizeUnit=B
MMTAppReg15.MEMORYMAP.StartAddress=0x30020100
MMTAppReg16.MEMORYMAP.AppRegionName=TxDescriptor
MMTAppReg16.MEMORYMAP.ContextLink=reserved
MMTAppReg16.MEMORYMAP.ContextName=CortexM4
MMTAppReg16.MEMORYMAP.CoreName=ARM Cortex-M4
MMTAppReg16.MEMORYMAP.IPParameters=StartAddress,Size,CoreName,SizeUnit,ContextName,Name,ContextLink,Shared,Shareability
MMTAppReg16.MEMORYMAP.Name=TxDescriptor
MMTAppReg16.MEMORYMAP.Shareability=Shareable
MMTAppReg16.MEMORYMAP.Shared=true
MMTAppReg16.MEMORYMAP.Size=128
MMTAppReg16.MEMORYMAP.SizeUnit=B
MMTAppReg16.MEMORYMAP.StartAddress=0x30020100
MMTAppReg17.MEMORYMAP.AppRegionName=RxPool
MMTAppReg17.MEMORYMAP.ContextLink=shared
MMTAppReg17.MEMORYMAP.ContextName=CortexM7
MMTAppReg17.MEMORYMAP.CoreName=ARM Cortex-M7
MMTAppReg17.MEMORYMAP.IPParameters=StartAddress,Size,CoreName,SizeUnit,ContextName,Name,ContextLink,Shareability,Shared
MMTAppReg17.MEMORYMAP.Name=RxPool
MMTAppReg17.MEMORYMAP.Shareability=Shareable
MMTAppReg17.MEMORYMAP.Shared=true
MMTAppReg17.MEMORYMAP.Size=1536
MMTAppReg17.MEMORYMAP.SizeUnit=B
MMTAppReg17.MEMORYMAP.StartAddress=0x30020200
MMTAppReg18.MEMORYMAP.AppRegionName=RxPool
MMTAppReg18.MEMORYMAP.ContextLink=reserved
MMTAppReg18.MEMORYMAP.ContextName=CortexM4
MMTAppReg18.MEMORYMAP.CoreName=ARM Cortex-M4
MMTAppReg18.MEMORYMAP.IPParameters=StartAddress,Size,CoreName,SizeUnit,ContextName,Name,ContextLink,Shared,Shareability
MMTAppReg18.MEMORYMAP.Name=RxPool
MMTAppReg18.MEMORYMAP.Shareability=Shareable
MMTAppReg18.MEMORYMAP.Shared=true
MMTAppReg18.MEMORYMAP.Size=1536
MMTAppReg18.MEMORYMAP.SizeUnit=B
MMTAppReg18.MEMORYMAP.StartAddress=0x30020200
MMTAppReg2.MEMORYMAP.AppRegionName=ITCMRAM
MMTAppReg2.MEMORYMAP.Cacheability=WTRA
MMTAppReg2.MEMORYMAP.ContextName=CortexM7
MMTAppReg2.MEMORYMAP.CoreName=ARM Cortex-M7
MMTAppReg2.MEMORYMAP.IPParameters=StartAddress,Size,CoreName,ContextName,Name,Cacheability
MMTAppReg2.MEMORYMAP.Name=ITCMRAM
MMTAppReg2.MEMORYMAP.Size=65536
MMTAppReg2.MEMORYMAP.StartAddress=0x00000000
MMTAppReg3.MEMORYMAP.AppRegionName=RAM_D1
MMTAppReg3.MEMORYMAP.ContextLink=shared
MMTAppReg3.MEMORYMAP.ContextName=CortexM7
MMTAppReg3.MEMORYMAP.CoreName=ARM Cortex-M7
MMTAppReg3.MEMORYMAP.IPParameters=StartAddress,Size,CoreName,ContextName,Name,ContextLink
MMTAppReg3.MEMORYMAP.Name=RAM_D1
MMTAppReg3.MEMORYMAP.Size=524288
MMTAppReg3.MEMORYMAP.StartAddress=0x24000000
MMTAppReg4.MEMORYMAP.AppRegionName=M7 non Shared Region
MMTAppReg4.MEMORYMAP.ContextLink=reserved
MMTAppReg4.MEMORYMAP.ContextName=CortexM4
MMTAppReg4.MEMORYMAP.CoreName=ARM Cortex-M4
MMTAppReg4.MEMORYMAP.IPParameters=StartAddress,Size,CoreName,ContextName,Name,ReservedRegion,ContextLink
MMTAppReg4.MEMORYMAP.Name=M7 non Shared Region
MMTAppReg4.MEMORYMAP.ReservedRegion=true
MMTAppReg4.MEMORYMAP.Size=524288
MMTAppReg4.MEMORYMAP.StartAddress=0x24000000
MMTAppReg5.MEMORYMAP.AP=RO_priv_only
MMTAppReg5.MEMORYMAP.AppRegionName=FLASH
MMTAppReg5.MEMORYMAP.Cacheability=WTRA
MMTAppReg5.MEMORYMAP.ContextLink=shared
MMTAppReg5.MEMORYMAP.ContextName=CortexM7
MMTAppReg5.MEMORYMAP.CoreName=ARM Cortex-M7
MMTAppReg5.MEMORYMAP.DefaultCodeRegion=true
MMTAppReg5.MEMORYMAP.IPParameters=StartAddress,Size,CoreName,MemType,ContextName,Name,AP,Cacheability,DefaultCodeRegion,ISRRegion,RootBootRegion,ContextLink
MMTAppReg5.MEMORYMAP.ISRRegion=true
MMTAppReg5.MEMORYMAP.MemType=ROM
MMTAppReg5.MEMORYMAP.Name=FLASH
MMTAppReg5.MEMORYMAP.RootBootRegion=true
MMTAppReg5.MEMORYMAP.Size=1048576
MMTAppReg5.MEMORYMAP.StartAddress=0x08000000
MMTAppReg6.MEMORYMAP.AppRegionName=M7 non Shared Region
MMTAppReg6.MEMORYMAP.ContextLink=reserved
MMTAppReg6.MEMORYMAP.ContextName=CortexM4
MMTAppReg6.MEMORYMAP.CoreName=ARM Cortex-M4
MMTAppReg6.MEMORYMAP.IPParameters=StartAddress,Size,CoreName,MemType,ContextName,Name,ReservedRegion,ContextLink
MMTAppReg6.MEMORYMAP.MemType=ROM
MMTAppReg6.MEMORYMAP.Name=M7 non Shared Region
MMTAppReg6.MEMORYMAP.ReservedRegion=true
MMTAppReg6.MEMORYMAP.Size=1048576
MMTAppReg6.MEMORYMAP.StartAddress=0x08000000
MMTAppReg7.MEMORYMAP.AppRegionName=RAM
MMTAppReg7.MEMORYMAP.ContextLink=shared
MMTAppReg7.MEMORYMAP.ContextName=CortexM4
MMTAppReg7.MEMORYMAP.CoreName=ARM Cortex-M4
MMTAppReg7.MEMORYMAP.DefaultDataRegion=true
MMTAppReg7.MEMORYMAP.IPParameters=StartAddress,Size,CoreName,ContextName,Name,DefaultDataRegion,ContextLink
MMTAppReg7.MEMORYMAP.Name=RAM
MMTAppReg7.MEMORYMAP.Size=294912
MMTAppReg7.MEMORYMAP.StartAddress=0x10000000
MMTAppReg8.MEMORYMAP.AppRegionName=M4 non Shared Region
MMTAppReg8.MEMORYMAP.ContextLink=reserved
MMTAppReg8.MEMORYMAP.ContextName=CortexM7
MMTAppReg8.MEMORYMAP.CoreName=ARM Cortex-M7
MMTAppReg8.MEMORYMAP.IPParameters=StartAddress,Size,CoreName,ContextName,Name,ReservedRegion,ContextLink
MMTAppReg8.MEMORYMAP.Name=M4 non Shared Region
MMTAppReg8.MEMORYMAP.ReservedRegion=true
MMTAppReg8.MEMORYMAP.Size=294912
MMTAppReg8.MEMORYMAP.StartAddress=0x10000000
MMTAppReg9.MEMORYMAP.AP=RO_priv_only
MMTAppReg9.MEMORYMAP.AppRegionName=FLASH
MMTAppReg9.MEMORYMAP.ContextLink=shared
MMTAppReg9.MEMORYMAP.ContextName=CortexM4
MMTAppReg9.MEMORYMAP.CoreName=ARM Cortex-M4
MMTAppReg9.MEMORYMAP.DefaultCodeRegion=true
MMTAppReg9.MEMORYMAP.IPParameters=StartAddress,Size,CoreName,MemType,ContextName,Name,AP,DefaultCodeRegion,ISRRegion,RootBootRegion,ContextLink
MMTAppReg9.MEMORYMAP.ISRRegion=true
MMTAppReg9.MEMORYMAP.MemType=ROM
MMTAppReg9.MEMORYMAP.Name=FLASH
MMTAppReg9.MEMORYMAP.RootBootRegion=true
MMTAppReg9.MEMORYMAP.Size=1048576
MMTAppReg9.MEMORYMAP.StartAddress=0x08100000
MMTAppRegionsCount=18
MMTConfigApplied=false
Mcu.CPN=STM32H757XIH6
Mcu.Context0=CortexM7
Mcu.Context1=CortexM4
Mcu.ContextNb=2
Mcu.Family=STM32H7
Mcu.IP0=ADC1
Mcu.IP1=ADC3
Mcu.IP10=FDCAN1
Mcu.IP11=FMC
Mcu.IP12=FREERTOS_M7
Mcu.IP13=I2C1
Mcu.IP14=I2C3
Mcu.IP15=I2S2
Mcu.IP16=LPTIM1
Mcu.IP17=LTDC
Mcu.IP18=LWIP
Mcu.IP19=MEMORYMAP
Mcu.IP2=CORTEX_M4
Mcu.IP20=NVIC1
Mcu.IP21=NVIC2
Mcu.IP22=QUADSPI
Mcu.IP23=RCC
Mcu.IP24=SDMMC1
Mcu.IP25=SYS_M4
Mcu.IP26=SYS
Mcu.IP27=USART1
Mcu.IP28=USART2
Mcu.IP29=USART6
Mcu.IP3=CORTEX_M7
Mcu.IP30=USB_HOST_M7
Mcu.IP31=USB_OTG_FS
Mcu.IP32=USB_OTG_HS
Mcu.IP4=DCMI
Mcu.IP5=DMA
Mcu.IP6=DMA2D
Mcu.IP7=DSIHOST
Mcu.IP8=ETH
Mcu.IP9=FATFS_M7
Mcu.IPNb=33
Mcu.Name=STM32H757XIHx
Mcu.Package=TFBGA240
Mcu.Pin0=PI6
Mcu.Pin1=PI5
Mcu.Pin10=PI1
Mcu.Pin100=PJ9
Mcu.Pin101=DSI_D0P
Mcu.Pin102=DSI_D0N
Mcu.Pin103=PH2
Mcu.Pin104=PA2
Mcu.Pin105=PA1
Mcu.Pin106=PA0
Mcu.Pin107=PJ0
Mcu.Pin108=PE10
Mcu.Pin109=PJ8
Mcu.Pin11=PI0
Mcu.Pin110=PJ7
Mcu.Pin111=PJ6
Mcu.Pin112=PH3
Mcu.Pin113=PH4
Mcu.Pin114=PH5
Mcu.Pin115=PI15
Mcu.Pin116=PJ1
Mcu.Pin117=PF13
Mcu.Pin118=PF14
Mcu.Pin119=PE9
Mcu.Pin12=PI7
Mcu.Pin120=PE11
Mcu.Pin121=PB10
Mcu.Pin122=PB11
Mcu.Pin123=PH10
Mcu.Pin124=PH11
Mcu.Pin125=PD15
Mcu.Pin126=PD14
Mcu.Pin127=PC2_C
Mcu.Pin128=PC3_C
Mcu.Pin129=PA6
Mcu.Pin13=PE1
Mcu.Pin130=PA7
Mcu.Pin131=PB2
Mcu.Pin132=PF12
Mcu.Pin133=PF15
Mcu.Pin134=PE12
Mcu.Pin135=PE15
Mcu.Pin136=PJ5
Mcu.Pin137=PH9
Mcu.Pin138=PH12
Mcu.Pin139=PD11
Mcu.Pin14=PB6
Mcu.Pin140=PD12
Mcu.Pin141=PD13
Mcu.Pin142=PA0_C
Mcu.Pin143=PA1_C
Mcu.Pin144=PA5
Mcu.Pin145=PC4
Mcu.Pin146=PB1
Mcu.Pin147=PJ2
Mcu.Pin148=PF11
Mcu.Pin149=PG0
Mcu.Pin15=PK4
Mcu.Pin150=PE8
Mcu.Pin151=PE13
Mcu.Pin152=PH6
Mcu.Pin153=PH8
Mcu.Pin154=PB15
Mcu.Pin155=PD10
Mcu.Pin156=PD9
Mcu.Pin157=PA4
Mcu.Pin158=PC5
Mcu.Pin159=PB0
Mcu.Pin16=PG11
Mcu.Pin160=PJ3
Mcu.Pin161=PJ4
Mcu.Pin162=PG1
Mcu.Pin163=PE7
Mcu.Pin164=PE14
Mcu.Pin165=PH7
Mcu.Pin166=PB13
Mcu.Pin167=PB14
Mcu.Pin168=PD8
Mcu.Pin169=VP_DMA2D_VS_DMA2D
Mcu.Pin17=PJ15
Mcu.Pin170=VP_FATFS_M7_VS_SDIO
Mcu.Pin171=VP_FREERTOS_M7_VS_CMSIS_V2
Mcu.Pin172=VP_LPTIM1_VS_LPTIM_counterModeInternalClock
Mcu.Pin173=VP_LTDC_DSIMode
Mcu.Pin174=VP_LWIP_VS_Enabled
Mcu.Pin175=VP_SYS_VS_tim15
Mcu.Pin176=VP_SYS_M4_VS_Systick
Mcu.Pin177=VP_USB_HOST_M7_VS_USB_HOST_MSC_HS
Mcu.Pin178=VP_USB_HOST_M7_VS_USB_HOST_MSC_FS
Mcu.Pin179=VP_MEMORYMAP_VS_MEMORYMAP
Mcu.Pin18=PD6
Mcu.Pin19=PD3
Mcu.Pin2=PI4
Mcu.Pin20=PC11
Mcu.Pin21=PI2
Mcu.Pin22=PH15
Mcu.Pin23=PH14
Mcu.Pin24=PC15-OSC32_OUT (OSC32_OUT)
Mcu.Pin25=PC14-OSC32_IN (OSC32_IN)
Mcu.Pin26=PE2
Mcu.Pin27=PE0
Mcu.Pin28=PB7
Mcu.Pin29=PK6
Mcu.Pin3=PB5
Mcu.Pin30=PK3
Mcu.Pin31=PG12
Mcu.Pin32=PD7
Mcu.Pin33=PC12
Mcu.Pin34=PI3
Mcu.Pin35=PE5
Mcu.Pin36=PE4
Mcu.Pin37=PE3
Mcu.Pin38=PB9
Mcu.Pin39=PB8
Mcu.Pin4=PK5
Mcu.Pin40=PG15
Mcu.Pin41=PK7
Mcu.Pin42=PG14
Mcu.Pin43=PG13
Mcu.Pin44=PJ14
Mcu.Pin45=PJ12
Mcu.Pin46=PD2
Mcu.Pin47=PD0
Mcu.Pin48=PA9
Mcu.Pin49=PH13
Mcu.Pin5=PG10
Mcu.Pin50=PI9
Mcu.Pin51=PI8
Mcu.Pin52=PE6
Mcu.Pin53=PJ13
Mcu.Pin54=PD1
Mcu.Pin55=PC8
Mcu.Pin56=PC9
Mcu.Pin57=PA8
Mcu.Pin58=PA12
Mcu.Pin59=PA11
Mcu.Pin6=PG9
Mcu.Pin60=PI10
Mcu.Pin61=PI11
Mcu.Pin62=PC7
Mcu.Pin63=PC6
Mcu.Pin64=PG8
Mcu.Pin65=PG7
Mcu.Pin66=PF2
Mcu.Pin67=PF1
Mcu.Pin68=PF0
Mcu.Pin69=PG5
Mcu.Pin7=PD5
Mcu.Pin70=PG6
Mcu.Pin71=PI12
Mcu.Pin72=PI13
Mcu.Pin73=PI14
Mcu.Pin74=PF3
Mcu.Pin75=PG4
Mcu.Pin76=PG3
Mcu.Pin77=PG2
Mcu.Pin78=PK2
Mcu.Pin79=PH1-OSC_OUT (PH1)
Mcu.Pin8=PD4
Mcu.Pin80=PH0-OSC_IN (PH0)
Mcu.Pin81=PF5
Mcu.Pin82=PF4
Mcu.Pin83=PK0
Mcu.Pin84=PK1
Mcu.Pin85=PF6
Mcu.Pin86=PF7
Mcu.Pin87=PF8
Mcu.Pin88=PJ11
Mcu.Pin89=DSI_D1P
Mcu.Pin9=PC10
Mcu.Pin90=DSI_D1N
Mcu.Pin91=PC0
Mcu.Pin92=PF10
Mcu.Pin93=PF9
Mcu.Pin94=PJ10
Mcu.Pin95=DSI_CKP
Mcu.Pin96=DSI_CKN
Mcu.Pin97=PC1
Mcu.Pin98=PC2
Mcu.Pin99=PC3
Mcu.PinsNb=180
Mcu.ThirdPartyNb=0
Mcu.UserConstants=
Mcu.UserName=STM32H757XIHx
MxCube.Version=6.13.0
MxDb.Version=DB.6.0.130
NVIC1.BusFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
NVIC1.DCMI_IRQn=true\:5\:0\:false\:false\:true\:true\:true\:true\:true
NVIC1.DMA1_Stream0_IRQn=true\:5\:0\:false\:false\:true\:true\:false\:true\:true
NVIC1.DMA1_Stream1_IRQn=true\:5\:0\:false\:false\:true\:true\:false\:true\:true
NVIC1.DMA1_Stream2_IRQn=true\:5\:0\:false\:false\:true\:true\:false\:true\:true
NVIC1.DMA1_Stream3_IRQn=true\:5\:0\:false\:false\:true\:true\:false\:true\:true
NVIC1.DMA1_Stream4_IRQn=true\:5\:0\:false\:false\:true\:true\:false\:true\:true
NVIC1.DebugMonitor_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
NVIC1.ETH_IRQn=true\:5\:0\:false\:false\:true\:true\:true\:true\:true
NVIC1.EXTI15_10_IRQn=true\:5\:0\:false\:false\:true\:true\:true\:true\:true
NVIC1.FDCAN1_IT0_IRQn=true\:5\:0\:false\:false\:true\:true\:true\:true\:true
NVIC1.FDCAN1_IT1_IRQn=true\:5\:0\:false\:false\:true\:true\:true\:true\:true
NVIC1.ForceEnableDMAVector=true
NVIC1.HardFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
NVIC1.LPTIM1_IRQn=true\:5\:0\:false\:false\:true\:true\:true\:true\:true
NVIC1.MemoryManagement_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
NVIC1.NonMaskableInt_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
NVIC1.OTG_FS_IRQn=true\:5\:0\:false\:false\:true\:true\:false\:true\:true
NVIC1.OTG_HS_IRQn=true\:5\:0\:false\:false\:true\:true\:false\:true\:true
NVIC1.PendSV_IRQn=true\:15\:0\:false\:false\:false\:true\:false\:false\:false
NVIC1.PriorityGroup=NVIC_PRIORITYGROUP_4
NVIC1.SDMMC1_IRQn=true\:5\:0\:false\:false\:true\:true\:true\:true\:true
NVIC1.SPI2_IRQn=true\:5\:0\:false\:false\:true\:true\:true\:true\:true
NVIC1.SVCall_IRQn=true\:0\:0\:false\:false\:false\:false\:false\:false\:false
NVIC1.SavedPendsvIrqHandlerGenerated=true
NVIC1.SavedSvcallIrqHandlerGenerated=true
NVIC1.SavedSystickIrqHandlerGenerated=true
NVIC1.SysTick_IRQn=true\:15\:0\:false\:false\:false\:true\:false\:false\:false
NVIC1.TIM15_IRQn=true\:15\:0\:false\:false\:true\:false\:false\:true\:true
NVIC1.TimeBase=TIM15_IRQn
NVIC1.TimeBaseIP=TIM15
NVIC1.USART2_IRQn=true\:5\:0\:false\:false\:true\:true\:true\:true\:true
NVIC1.USART6_IRQn=true\:5\:0\:false\:false\:true\:true\:true\:true\:true
NVIC1.UsageFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
NVIC2.BusFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC2.DebugMonitor_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC2.ForceEnableDMAVector=true
NVIC2.HardFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC2.MemoryManagement_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC2.NonMaskableInt_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC2.PendSV_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC2.PriorityGroup=NVIC_PRIORITYGROUP_4
NVIC2.SVCall_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC2.SysTick_IRQn=true\:15\:0\:false\:false\:true\:false\:true\:false
NVIC2.UsageFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
PA0.ContextOwner=CortexM7
PA0.GPIOParameters=GPIO_Label,PinAttribute
PA0.GPIO_Label=LED_YELLOW
PA0.Locked=true
PA0.PinAttribute=CortexM7
PA0.Signal=GPIO_Output
PA0_C.GPIOParameters=PinAttribute
PA0_C.Locked=true
PA0_C.PinAttribute=CortexM7
PA0_C.Signal=ADCx_INP0
PA1.GPIOParameters=GPIO_Speed,PinAttribute
PA1.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PA1.Mode=RMII
PA1.PinAttribute=CortexM7
PA1.Signal=ETH_REF_CLK
PA11.GPIOParameters=PinAttribute
PA11.Mode=Host_Only
PA11.PinAttribute=CortexM7
PA11.Signal=USB_OTG_FS_DM
PA12.GPIOParameters=PinAttribute
PA12.Mode=Host_Only
PA12.PinAttribute=CortexM7
PA12.Signal=USB_OTG_FS_DP
PA1_C.GPIOParameters=PinAttribute
PA1_C.PinAttribute=CortexM7
PA1_C.Signal=ADCx_INP1
PA2.GPIOParameters=GPIO_Speed,PinAttribute
PA2.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PA2.Mode=RMII
PA2.PinAttribute=CortexM7
PA2.Signal=ETH_MDIO
PA4.GPIOParameters=GPIO_Speed,PinAttribute
PA4.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PA4.Mode=Slave_8_bits_External_Synchro
PA4.PinAttribute=CortexM7
PA4.Signal=DCMI_HSYNC
PA5.ContextOwner=CortexM7
PA5.GPIOParameters=GPIO_Label,PinAttribute
PA5.GPIO_Label=LED_RED
PA5.Locked=true
PA5.PinAttribute=CortexM7
PA5.Signal=GPIO_Output
PA6.GPIOParameters=GPIO_Speed,PinAttribute
PA6.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PA6.Mode=Slave_8_bits_External_Synchro
PA6.PinAttribute=CortexM7
PA6.Signal=DCMI_PIXCLK
PA7.GPIOParameters=GPIO_Speed,PinAttribute
PA7.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PA7.Mode=RMII
PA7.PinAttribute=CortexM7
PA7.Signal=ETH_CRS_DV
PA8.GPIOParameters=GPIO_Speed,PinAttribute
PA8.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PA8.Mode=Clock-out-1
PA8.PinAttribute=Free
PA8.Signal=RCC_MCO_1
PA9.GPIOParameters=PinAttribute
PA9.Mode=Activate_VBUS
PA9.PinAttribute=CortexM7
PA9.Signal=USB_OTG_FS_VBUS
PB0.ContextOwner=CortexM7
PB0.GPIOParameters=GPIO_Label,PinAttribute
PB0.GPIO_Label=DISP_DSI_RESET
PB0.Locked=true
PB0.PinAttribute=CortexM7
PB0.Signal=GPIO_Output
PB1.ContextOwner=CortexM7
PB1.GPIOParameters=GPIO_Label,PinAttribute
PB1.GPIO_Label=USB_HS_VBUS_EN
PB1.Locked=true
PB1.PinAttribute=CortexM7
PB1.Signal=GPIO_Output
PB10.ContextOwner=CortexM7
PB10.GPIOParameters=GPIO_Label,GPIO_ModeDefaultEXTI,PinAttribute
PB10.GPIO_Label=TP_INT
PB10.GPIO_ModeDefaultEXTI=GPIO_MODE_IT_FALLING
PB10.Locked=true
PB10.PinAttribute=CortexM7
PB10.Signal=GPXTI10
PB11.ContextOwner=CortexM7
PB11.GPIOParameters=GPIO_Label,PinAttribute
PB11.GPIO_Label=DISP_BACKLIGHT_EN
PB11.Locked=true
PB11.PinAttribute=CortexM7
PB11.Signal=GPIO_Output
PB13.GPIOParameters=PinAttribute
PB13.Mode=Activate_VBUS_FS
PB13.PinAttribute=CortexM7
PB13.Signal=USB_OTG_HS_VBUS
PB14.GPIOParameters=PinAttribute
PB14.Mode=Host_FS
PB14.PinAttribute=CortexM7
PB14.Signal=USB_OTG_HS_DM
PB15.GPIOParameters=PinAttribute
PB15.Mode=Host_FS
PB15.PinAttribute=CortexM7
PB15.Signal=USB_OTG_HS_DP
PB2.ContextOwner=CortexM7
PB2.GPIOParameters=GPIO_Label,PinAttribute
PB2.GPIO_Label=USB_FS_VBUS_EN
PB2.Locked=true
PB2.PinAttribute=CortexM7
PB2.Signal=GPIO_Output
PB5.ContextOwner=CortexM7
PB5.GPIOParameters=PinAttribute
PB5.Locked=true
PB5.PinAttribute=CortexM7
PB5.Signal=GPIO_Input
PB6.GPIOParameters=PinAttribute
PB6.Locked=true
PB6.Mode=Asynchronous
PB6.PinAttribute=CortexM7
PB6.Signal=USART1_TX
PB7.GPIOParameters=PinAttribute
PB7.Locked=true
PB7.Mode=Asynchronous
PB7.PinAttribute=CortexM7
PB7.Signal=USART1_RX
PB8.GPIOParameters=GPIO_Speed,PinAttribute
PB8.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PB8.Mode=I2C
PB8.PinAttribute=CortexM7
PB8.Signal=I2C1_SCL
PB9.GPIOParameters=GPIO_Speed,PinAttribute
PB9.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PB9.Mode=I2C
PB9.PinAttribute=CortexM7
PB9.Signal=I2C1_SDA
PC0.GPIOParameters=PinAttribute
PC0.PinAttribute=CortexM7
PC0.Signal=FMC_SDNWE
PC1.GPIOParameters=GPIO_Speed,PinAttribute
PC1.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PC1.Mode=RMII
PC1.PinAttribute=CortexM7
PC1.Signal=ETH_MDC
PC10.GPIOParameters=PinAttribute
PC10.Mode=SD_4_bits_Wide_bus
PC10.PinAttribute=CortexM7
PC10.Signal=SDMMC1_D2
PC11.GPIOParameters=PinAttribute
PC11.Mode=SD_4_bits_Wide_bus
PC11.PinAttribute=CortexM7
PC11.Signal=SDMMC1_D3
PC12.GPIOParameters=PinAttribute
PC12.Mode=SD_4_bits_Wide_bus
PC12.PinAttribute=CortexM7
PC12.Signal=SDMMC1_CK
PC14-OSC32_IN\ (OSC32_IN).GPIOParameters=PinAttribute
PC14-OSC32_IN\ (OSC32_IN).Mode=LSE-External-Oscillator
PC14-OSC32_IN\ (OSC32_IN).PinAttribute=Free
PC14-OSC32_IN\ (OSC32_IN).Signal=RCC_OSC32_IN
PC15-OSC32_OUT\ (OSC32_OUT).GPIOParameters=PinAttribute
PC15-OSC32_OUT\ (OSC32_OUT).Mode=LSE-External-Oscillator
PC15-OSC32_OUT\ (OSC32_OUT).PinAttribute=Free
PC15-OSC32_OUT\ (OSC32_OUT).Signal=RCC_OSC32_OUT
PC2.GPIOParameters=PinAttribute
PC2.Mode=SdramChipSelect1_1
PC2.PinAttribute=CortexM7
PC2.Signal=FMC_SDNE0
PC2_C.GPIOParameters=PinAttribute
PC2_C.Locked=true
PC2_C.Mode=IN0-Single-Ended
PC2_C.PinAttribute=CortexM7
PC2_C.Signal=ADC3_INP0
PC3.GPIOParameters=PinAttribute
PC3.Mode=SdramChipSelect1_1
PC3.PinAttribute=CortexM7
PC3.Signal=FMC_SDCKE0
PC3_C.GPIOParameters=PinAttribute
PC3_C.Locked=true
PC3_C.Mode=IN1-Single-Ended
PC3_C.PinAttribute=CortexM7
PC3_C.Signal=ADC3_INP1
PC4.GPIOParameters=GPIO_Speed,PinAttribute
PC4.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PC4.Mode=RMII
PC4.PinAttribute=CortexM7
PC4.Signal=ETH_RXD0
PC5.GPIOParameters=GPIO_Speed,PinAttribute
PC5.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PC5.Mode=RMII
PC5.PinAttribute=CortexM7
PC5.Signal=ETH_RXD1
PC6.GPIOParameters=GPIO_Speed,PinAttribute
PC6.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PC6.Mode=Master_Clock_Activated
PC6.PinAttribute=CortexM7
PC6.Signal=I2S2_MCK
PC7.ContextOwner=CortexM7
PC7.GPIOParameters=GPIO_Label,PinAttribute
PC7.GPIO_Label=WIFI_WL_REG_ON
PC7.Locked=true
PC7.PinAttribute=CortexM7
PC7.Signal=GPIO_Output
PC8.GPIOParameters=PinAttribute
PC8.Mode=SD_4_bits_Wide_bus
PC8.PinAttribute=CortexM7
PC8.Signal=SDMMC1_D0
PC9.GPIOParameters=PinAttribute
PC9.Mode=SD_4_bits_Wide_bus
PC9.PinAttribute=CortexM7
PC9.Signal=SDMMC1_D1
PD0.GPIOParameters=PinAttribute
PD0.PinAttribute=CortexM7
PD0.Signal=FMC_D2_DA2
PD1.GPIOParameters=PinAttribute
PD1.PinAttribute=CortexM7
PD1.Signal=FMC_D3_DA3
PD10.GPIOParameters=PinAttribute
PD10.PinAttribute=CortexM7
PD10.Signal=FMC_D15_DA15
PD11.GPIOParameters=GPIO_Speed,PinAttribute
PD11.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PD11.Locked=true
PD11.Mode=Single Bank 1
PD11.PinAttribute=CortexM7
PD11.Signal=QUADSPI_BK1_IO0
PD12.GPIOParameters=GPIO_Speed,PinAttribute
PD12.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PD12.Locked=true
PD12.Mode=Single Bank 1
PD12.PinAttribute=CortexM7
PD12.Signal=QUADSPI_BK1_IO1
PD13.GPIOParameters=GPIO_Speed,PinAttribute
PD13.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PD13.Locked=true
PD13.Mode=Single Bank 1
PD13.PinAttribute=CortexM7
PD13.Signal=QUADSPI_BK1_IO3
PD14.GPIOParameters=PinAttribute
PD14.PinAttribute=CortexM7
PD14.Signal=FMC_D0_DA0
PD15.GPIOParameters=PinAttribute
PD15.PinAttribute=CortexM7
PD15.Signal=FMC_D1_DA1
PD2.GPIOParameters=PinAttribute
PD2.Mode=SD_4_bits_Wide_bus
PD2.PinAttribute=CortexM7
PD2.Signal=SDMMC1_CMD
PD3.GPIOParameters=PinAttribute
PD3.Mode=CTS_RTS
PD3.PinAttribute=CortexM7
PD3.Signal=USART2_CTS
PD4.GPIOParameters=PinAttribute
PD4.Mode=CTS_RTS
PD4.PinAttribute=CortexM7
PD4.Signal=USART2_RTS
PD5.GPIOParameters=PinAttribute
PD5.Mode=Asynchronous
PD5.PinAttribute=CortexM7
PD5.Signal=USART2_TX
PD6.GPIOParameters=PinAttribute
PD6.Mode=Asynchronous
PD6.PinAttribute=CortexM7
PD6.Signal=USART2_RX
PD7.ContextOwner=CortexM7
PD7.GPIOParameters=GPIO_Speed,GPIO_Label,PinAttribute
PD7.GPIO_Label=RS485_TX_EN
PD7.GPIO_Speed=GPIO_SPEED_FREQ_HIGH
PD7.Locked=true
PD7.PinAttribute=CortexM7
PD7.Signal=GPIO_Output
PD8.GPIOParameters=PinAttribute
PD8.PinAttribute=CortexM7
PD8.Signal=FMC_D13_DA13
PD9.GPIOParameters=PinAttribute
PD9.PinAttribute=CortexM7
PD9.Signal=FMC_D14_DA14
PE0.GPIOParameters=PinAttribute
PE0.PinAttribute=CortexM7
PE0.Signal=FMC_NBL0
PE1.GPIOParameters=PinAttribute
PE1.PinAttribute=CortexM7
PE1.Signal=FMC_NBL1
PE10.GPIOParameters=PinAttribute
PE10.PinAttribute=CortexM7
PE10.Signal=FMC_D7_DA7
PE11.GPIOParameters=PinAttribute
PE11.PinAttribute=CortexM7
PE11.Signal=FMC_D8_DA8
PE12.GPIOParameters=PinAttribute
PE12.PinAttribute=CortexM7
PE12.Signal=FMC_D9_DA9
PE13.GPIOParameters=PinAttribute
PE13.PinAttribute=CortexM7
PE13.Signal=FMC_D10_DA10
PE14.GPIOParameters=PinAttribute
PE14.PinAttribute=CortexM7
PE14.Signal=FMC_D11_DA11
PE15.GPIOParameters=PinAttribute
PE15.PinAttribute=CortexM7
PE15.Signal=FMC_D12_DA12
PE2.GPIOParameters=GPIO_Speed,PinAttribute
PE2.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PE2.Mode=Single Bank 1
PE2.PinAttribute=CortexM7
PE2.Signal=QUADSPI_BK1_IO2
PE3.ContextOwner=CortexM7
PE3.GPIOParameters=PinState,GPIO_Label,PinAttribute
PE3.GPIO_Label=CAMERA_RESET
PE3.Locked=true
PE3.PinAttribute=CortexM7
PE3.PinState=GPIO_PIN_SET
PE3.Signal=GPIO_Output
PE4.GPIOParameters=GPIO_Speed,PinAttribute
PE4.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PE4.Locked=true
PE4.Mode=Slave_8_bits_External_Synchro
PE4.PinAttribute=CortexM7
PE4.Signal=DCMI_D4
PE5.ContextOwner=CortexM7
PE5.GPIOParameters=GPIO_Label,PinAttribute
PE5.GPIO_Label=LED_SYS
PE5.Locked=true
PE5.PinAttribute=CortexM7
PE5.Signal=GPIO_Output
PE6.ContextOwner=CortexM7
PE6.GPIOParameters=GPIO_Label,PinAttribute
PE6.GPIO_Label=LED_AMBER
PE6.Locked=true
PE6.PinAttribute=CortexM7
PE6.Signal=GPIO_Output
PE7.GPIOParameters=PinAttribute
PE7.PinAttribute=CortexM7
PE7.Signal=FMC_D4_DA4
PE8.GPIOParameters=PinAttribute
PE8.PinAttribute=CortexM7
PE8.Signal=FMC_D5_DA5
PE9.GPIOParameters=PinAttribute
PE9.PinAttribute=CortexM7
PE9.Signal=FMC_D6_DA6
PF0.GPIOParameters=PinAttribute
PF0.PinAttribute=CortexM7
PF0.Signal=FMC_A0
PF1.GPIOParameters=PinAttribute
PF1.PinAttribute=CortexM7
PF1.Signal=FMC_A1
PF10.GPIOParameters=GPIO_Speed,PinAttribute
PF10.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PF10.Mode=Single Bank 1
PF10.PinAttribute=CortexM7
PF10.Signal=QUADSPI_CLK
PF11.GPIOParameters=PinAttribute
PF11.PinAttribute=CortexM7
PF11.Signal=FMC_SDNRAS
PF12.GPIOParameters=PinAttribute
PF12.PinAttribute=CortexM7
PF12.Signal=FMC_A6
PF13.GPIOParameters=PinAttribute
PF13.PinAttribute=CortexM7
PF13.Signal=FMC_A7
PF14.GPIOParameters=PinAttribute
PF14.PinAttribute=CortexM7
PF14.Signal=FMC_A8
PF15.GPIOParameters=PinAttribute
PF15.PinAttribute=CortexM7
PF15.Signal=FMC_A9
PF2.GPIOParameters=PinAttribute
PF2.PinAttribute=CortexM7
PF2.Signal=FMC_A2
PF3.GPIOParameters=PinAttribute
PF3.PinAttribute=CortexM7
PF3.Signal=FMC_A3
PF4.GPIOParameters=PinAttribute
PF4.PinAttribute=CortexM7
PF4.Signal=FMC_A4
PF5.GPIOParameters=PinAttribute
PF5.PinAttribute=CortexM7
PF5.Signal=FMC_A5
PF6.ContextOwner=CortexM7
PF6.GPIOParameters=PinAttribute
PF6.Locked=true
PF6.PinAttribute=CortexM7
PF6.Signal=GPIO_Output
PF7.ContextOwner=CortexM7
PF7.GPIOParameters=PinAttribute
PF7.Locked=true
PF7.PinAttribute=CortexM7
PF7.Signal=GPIO_Input
PF8.ContextOwner=CortexM7
PF8.GPIOParameters=PinAttribute
PF8.Locked=true
PF8.PinAttribute=CortexM7
PF8.Signal=GPIO_Input
PF9.ContextOwner=CortexM7
PF9.GPIOParameters=PinAttribute
PF9.Locked=true
PF9.PinAttribute=CortexM7
PF9.Signal=GPIO_Output
PG0.GPIOParameters=PinAttribute
PG0.PinAttribute=CortexM7
PG0.Signal=FMC_A10
PG1.GPIOParameters=PinAttribute
PG1.PinAttribute=CortexM7
PG1.Signal=FMC_A11
PG10.GPIOParameters=GPIO_Speed,PinAttribute
PG10.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PG10.Mode=Slave_8_bits_External_Synchro
PG10.PinAttribute=CortexM7
PG10.Signal=DCMI_D2
PG11.GPIOParameters=GPIO_Speed,PinAttribute
PG11.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PG11.Mode=RMII
PG11.PinAttribute=CortexM7
PG11.Signal=ETH_TX_EN
PG12.GPIOParameters=GPIO_Speed,PinAttribute
PG12.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PG12.Mode=RMII
PG12.PinAttribute=CortexM7
PG12.Signal=ETH_TXD1
PG13.GPIOParameters=GPIO_Speed,PinAttribute
PG13.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PG13.Mode=RMII
PG13.PinAttribute=CortexM7
PG13.Signal=ETH_TXD0
PG14.GPIOParameters=GPIO_Speed,PinAttribute
PG14.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PG14.Mode=Asynchronous
PG14.PinAttribute=CortexM7
PG14.Signal=USART6_TX
PG15.GPIOParameters=PinAttribute
PG15.PinAttribute=CortexM7
PG15.Signal=FMC_SDNCAS
PG2.GPIOParameters=PinAttribute
PG2.PinAttribute=CortexM7
PG2.Signal=FMC_A12
PG3.ContextOwner=CortexM7
PG3.GPIOParameters=GPIO_Label,PinAttribute
PG3.GPIO_Label=ENET_INT
PG3.Locked=true
PG3.PinAttribute=CortexM7
PG3.Signal=GPXTI3
PG4.GPIOParameters=PinAttribute
PG4.PinAttribute=CortexM7
PG4.Signal=FMC_A14_BA0
PG5.GPIOParameters=PinAttribute
PG5.PinAttribute=CortexM7
PG5.Signal=FMC_A15_BA1
PG6.GPIOParameters=GPIO_Speed,PinAttribute
PG6.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PG6.Mode=Single Bank 1
PG6.PinAttribute=CortexM7
PG6.Signal=QUADSPI_BK1_NCS
PG7.GPIOParameters=GPIO_Speed,PinAttribute
PG7.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PG7.Locked=true
PG7.PinAttribute=CortexM7
PG7.Signal=LTDC_CLK
PG8.GPIOParameters=PinAttribute
PG8.PinAttribute=CortexM7
PG8.Signal=FMC_SDCLK
PG9.GPIOParameters=GPIO_Speed,PinAttribute
PG9.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PG9.Mode=Asynchronous
PG9.PinAttribute=CortexM7
PG9.Signal=USART6_RX
PH0-OSC_IN\ (PH0).GPIOParameters=PinAttribute
PH0-OSC_IN\ (PH0).Mode=HSE-External-Oscillator
PH0-OSC_IN\ (PH0).PinAttribute=Free
PH0-OSC_IN\ (PH0).Signal=RCC_OSC_IN
PH1-OSC_OUT\ (PH1).GPIOParameters=PinAttribute
PH1-OSC_OUT\ (PH1).Mode=HSE-External-Oscillator
PH1-OSC_OUT\ (PH1).PinAttribute=Free
PH1-OSC_OUT\ (PH1).Signal=RCC_OSC_OUT
PH10.GPIOParameters=GPIO_Speed,PinAttribute
PH10.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PH10.Locked=true
PH10.Mode=Slave_8_bits_External_Synchro
PH10.PinAttribute=CortexM7
PH10.Signal=DCMI_D1
PH11.ContextOwner=CortexM7
PH11.GPIOParameters=GPIO_Label,PinAttribute
PH11.GPIO_Label=DISP_PWM
PH11.Locked=true
PH11.PinAttribute=CortexM7
PH11.Signal=GPIO_Output
PH12.GPIOParameters=GPIO_Speed,PinAttribute
PH12.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PH12.Locked=true
PH12.Mode=Slave_8_bits_External_Synchro
PH12.PinAttribute=CortexM7
PH12.Signal=DCMI_D3
PH13.GPIOParameters=GPIO_Speed,PinAttribute
PH13.GPIO_Speed=GPIO_SPEED_FREQ_HIGH
PH13.Locked=true
PH13.Mode=FDCAN_Activate
PH13.PinAttribute=CortexM7
PH13.Signal=FDCAN1_TX
PH14.GPIOParameters=GPIO_Speed,PinAttribute
PH14.GPIO_Speed=GPIO_SPEED_FREQ_HIGH
PH14.Mode=FDCAN_Activate
PH14.PinAttribute=CortexM7
PH14.Signal=FDCAN1_RX
PH15.ContextOwner=CortexM7
PH15.GPIOParameters=PinState,GPIO_Label,PinAttribute
PH15.GPIO_Label=ENET_RST
PH15.Locked=true
PH15.PinAttribute=CortexM7
PH15.PinState=GPIO_PIN_SET
PH15.Signal=GPIO_Output
PH2.ContextOwner=CortexM7
PH2.GPIOParameters=GPIO_PuPd,GPIO_Label,PinAttribute,GPIO_Mode
PH2.GPIO_Label=BUTTON_H2
PH2.GPIO_Mode=GPIO_MODE_INPUT
PH2.GPIO_PuPd=GPIO_PULLUP
PH2.Locked=true
PH2.PinAttribute=CortexM7
PH2.Signal=GPIO_Input
PH3.ContextOwner=CortexM7
PH3.GPIOParameters=GPIO_PuPd,GPIO_Label,PinAttribute,GPIO_Mode
PH3.GPIO_Label=BUTTON_H3
PH3.GPIO_Mode=GPIO_MODE_INPUT
PH3.GPIO_PuPd=GPIO_PULLUP
PH3.Locked=true
PH3.PinAttribute=CortexM7
PH3.Signal=GPIO_Input
PH4.ContextOwner=CortexM7
PH4.GPIOParameters=GPIO_PuPd,GPIO_Label,PinAttribute,GPIO_Mode
PH4.GPIO_Label=BUTTON_H4
PH4.GPIO_Mode=GPIO_MODE_INPUT
PH4.GPIO_PuPd=GPIO_PULLUP
PH4.Locked=true
PH4.PinAttribute=CortexM7
PH4.Signal=GPIO_Input
PH5.ContextOwner=CortexM7
PH5.GPIOParameters=GPIO_PuPd,GPIO_Label,PinAttribute,GPIO_Mode
PH5.GPIO_Label=BUTTON_H5
PH5.GPIO_Mode=GPIO_MODE_INPUT
PH5.GPIO_PuPd=GPIO_PULLUP
PH5.Locked=true
PH5.PinAttribute=CortexM7
PH5.Signal=GPIO_Input
PH6.ContextOwner=CortexM7
PH6.GPIOParameters=GPIO_Label,PinAttribute
PH6.GPIO_Label=TP_RST
PH6.Locked=true
PH6.PinAttribute=CortexM7
PH6.Signal=GPIO_Output
PH7.GPIOParameters=GPIO_Speed,PinAttribute
PH7.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PH7.Locked=true
PH7.Mode=I2C
PH7.PinAttribute=CortexM7
PH7.Signal=I2C3_SCL
PH8.GPIOParameters=GPIO_Speed,PinAttribute
PH8.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PH8.Locked=true
PH8.Mode=I2C
PH8.PinAttribute=CortexM7
PH8.Signal=I2C3_SDA
PH9.GPIOParameters=GPIO_Speed,PinAttribute
PH9.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PH9.Locked=true
PH9.Mode=Slave_8_bits_External_Synchro
PH9.PinAttribute=CortexM7
PH9.Signal=DCMI_D0
PI0.GPIOParameters=GPIO_Speed,PinAttribute
PI0.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PI0.Mode=Full_Duplex_Master
PI0.PinAttribute=CortexM7
PI0.Signal=I2S2_WS
PI1.GPIOParameters=GPIO_Speed,PinAttribute
PI1.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PI1.Mode=Full_Duplex_Master
PI1.PinAttribute=CortexM7
PI1.Signal=I2S2_CK
PI10.ContextOwner=CortexM7
PI10.GPIOParameters=PinAttribute
PI10.Locked=true
PI10.PinAttribute=CortexM7
PI10.Signal=GPIO_Output
PI11.ContextOwner=CortexM7
PI11.GPIOParameters=GPIO_Label,PinAttribute
PI11.GPIO_Label=LED_GREEN
PI11.Locked=true
PI11.PinAttribute=CortexM7
PI11.Signal=GPIO_Output
PI12.GPIOParameters=GPIO_Speed,PinAttribute
PI12.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PI12.Locked=true
PI12.PinAttribute=CortexM7
PI12.Signal=LTDC_HSYNC
PI13.GPIOParameters=GPIO_Speed,PinAttribute
PI13.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PI13.Locked=true
PI13.PinAttribute=CortexM7
PI13.Signal=LTDC_VSYNC
PI14.ContextOwner=CortexM7
PI14.GPIOParameters=GPIO_Label,PinAttribute
PI14.GPIO_Label=SDCARD_DETECT
PI14.Locked=true
PI14.PinAttribute=CortexM7
PI14.Signal=GPIO_Input
PI15.GPIOParameters=GPIO_Speed,PinAttribute
PI15.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PI15.Locked=true
PI15.PinAttribute=CortexM7
PI15.Signal=LTDC_R0
PI2.GPIOParameters=GPIO_Speed,PinAttribute
PI2.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PI2.Mode=Full_Duplex_Master
PI2.PinAttribute=CortexM7
PI2.Signal=I2S2_SDI
PI3.GPIOParameters=GPIO_Speed,PinAttribute
PI3.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PI3.Mode=Full_Duplex_Master
PI3.PinAttribute=CortexM7
PI3.Signal=I2S2_SDO
PI4.GPIOParameters=GPIO_Speed,PinAttribute
PI4.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PI4.Mode=Slave_8_bits_External_Synchro
PI4.PinAttribute=CortexM7
PI4.Signal=DCMI_D5
PI5.GPIOParameters=GPIO_Speed,PinAttribute
PI5.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PI5.Mode=Slave_8_bits_External_Synchro
PI5.PinAttribute=CortexM7
PI5.Signal=DCMI_VSYNC
PI6.GPIOParameters=GPIO_Speed,PinAttribute
PI6.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PI6.Mode=Slave_8_bits_External_Synchro
PI6.PinAttribute=CortexM7
PI6.Signal=DCMI_D6
PI7.GPIOParameters=GPIO_Speed,PinAttribute
PI7.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PI7.Mode=Slave_8_bits_External_Synchro
PI7.PinAttribute=CortexM7
PI7.Signal=DCMI_D7
PI8.ContextOwner=CortexM7
PI8.GPIOParameters=GPIO_Label,PinAttribute
PI8.GPIO_Label=CYBSP_BT_POWER
PI8.Locked=true
PI8.PinAttribute=CortexM7
PI8.Signal=GPIO_Output
PI9.ContextOwner=CortexM7
PI9.GPIOParameters=PinAttribute
PI9.Locked=true
PI9.PinAttribute=CortexM7
PI9.Signal=GPIO_Input
PJ0.GPIOParameters=GPIO_Speed,PinAttribute
PJ0.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PJ0.Locked=true
PJ0.PinAttribute=CortexM7
PJ0.Signal=LTDC_R1
PJ1.GPIOParameters=GPIO_Speed,PinAttribute
PJ1.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PJ1.Locked=true
PJ1.PinAttribute=CortexM7
PJ1.Signal=LTDC_R2
PJ10.GPIOParameters=GPIO_Speed,PinAttribute
PJ10.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PJ10.Locked=true
PJ10.PinAttribute=CortexM7
PJ10.Signal=LTDC_G3
PJ11.GPIOParameters=GPIO_Speed,PinAttribute
PJ11.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PJ11.Locked=true
PJ11.PinAttribute=CortexM7
PJ11.Signal=LTDC_G4
PJ12.GPIOParameters=GPIO_Speed,PinAttribute
PJ12.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PJ12.Locked=true
PJ12.PinAttribute=CortexM7
PJ12.Signal=LTDC_B0
PJ13.GPIOParameters=GPIO_Speed,PinAttribute
PJ13.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PJ13.Locked=true
PJ13.PinAttribute=CortexM7
PJ13.Signal=LTDC_B1
PJ14.GPIOParameters=GPIO_Speed,PinAttribute
PJ14.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PJ14.Locked=true
PJ14.PinAttribute=CortexM7
PJ14.Signal=LTDC_B2
PJ15.GPIOParameters=GPIO_Speed,PinAttribute
PJ15.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PJ15.Locked=true
PJ15.PinAttribute=CortexM7
PJ15.Signal=LTDC_B3
PJ2.GPIOParameters=GPIO_Speed,PinAttribute
PJ2.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PJ2.Locked=true
PJ2.PinAttribute=CortexM7
PJ2.Signal=LTDC_R3
PJ3.GPIOParameters=GPIO_Speed,PinAttribute
PJ3.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PJ3.Locked=true
PJ3.PinAttribute=CortexM7
PJ3.Signal=LTDC_R4
PJ4.GPIOParameters=GPIO_Speed,PinAttribute
PJ4.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PJ4.Locked=true
PJ4.PinAttribute=CortexM7
PJ4.Signal=LTDC_R5
PJ5.GPIOParameters=GPIO_Speed,PinAttribute
PJ5.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PJ5.Locked=true
PJ5.PinAttribute=CortexM7
PJ5.Signal=LTDC_R6
PJ6.GPIOParameters=GPIO_Speed,PinAttribute
PJ6.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PJ6.Locked=true
PJ6.PinAttribute=CortexM7
PJ6.Signal=LTDC_R7
PJ7.GPIOParameters=GPIO_Speed,PinAttribute
PJ7.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PJ7.Locked=true
PJ7.PinAttribute=CortexM7
PJ7.Signal=LTDC_G0
PJ8.GPIOParameters=GPIO_Speed,PinAttribute
PJ8.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PJ8.Locked=true
PJ8.PinAttribute=CortexM7
PJ8.Signal=LTDC_G1
PJ9.GPIOParameters=GPIO_Speed,PinAttribute
PJ9.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PJ9.Locked=true
PJ9.PinAttribute=CortexM7
PJ9.Signal=LTDC_G2
PK0.GPIOParameters=GPIO_Speed,PinAttribute
PK0.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PK0.Locked=true
PK0.PinAttribute=CortexM7
PK0.Signal=LTDC_G5
PK1.GPIOParameters=GPIO_Speed,PinAttribute
PK1.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PK1.Locked=true
PK1.PinAttribute=CortexM7
PK1.Signal=LTDC_G6
PK2.GPIOParameters=GPIO_Speed,PinAttribute
PK2.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PK2.Locked=true
PK2.PinAttribute=CortexM7
PK2.Signal=LTDC_G7
PK3.GPIOParameters=GPIO_Speed,PinAttribute
PK3.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PK3.Locked=true
PK3.PinAttribute=CortexM7
PK3.Signal=LTDC_B4
PK4.GPIOParameters=GPIO_Speed,PinAttribute
PK4.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PK4.Locked=true
PK4.PinAttribute=CortexM7
PK4.Signal=LTDC_B5
PK5.GPIOParameters=GPIO_Speed,PinAttribute
PK5.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PK5.Locked=true
PK5.PinAttribute=CortexM7
PK5.Signal=LTDC_B6
PK6.GPIOParameters=GPIO_Speed,PinAttribute
PK6.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PK6.Locked=true
PK6.PinAttribute=CortexM7
PK6.Signal=LTDC_B7
PK7.GPIOParameters=GPIO_Speed,PinAttribute
PK7.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PK7.Locked=true
PK7.PinAttribute=CortexM7
PK7.Signal=LTDC_DE
PinOutPanel.CurrentBGAView=Top
PinOutPanel.RotationAngle=0
ProjectManager.AskForMigrate=true
ProjectManager.BackupPrevious=false
ProjectManager.BootMode=boot0
ProjectManager.CompilerOptimize=6
ProjectManager.ComputerToolchain=false
ProjectManager.CoupleFile=false
ProjectManager.CustomerFirmwarePackage=
ProjectManager.DefaultFWLocation=true
ProjectManager.DeletePrevious=true
ProjectManager.DeviceId=STM32H757XIHx
ProjectManager.FirmwarePackage=STM32Cube FW_H7 V1.12.1
ProjectManager.FreePins=false
ProjectManager.HalAssertFull=false
ProjectManager.HeapSize=M4-0x200,M7-0x200
ProjectManager.KeepUserCode=true
ProjectManager.LastFirmware=true
ProjectManager.LibraryCopy=1
ProjectManager.MainLocation=Core/Src
ProjectManager.NoMain=false
ProjectManager.PreviousToolchain=
ProjectManager.ProjectBuild=false
ProjectManager.ProjectFileName=starsom-stm32h757-tester.ioc
ProjectManager.ProjectName=starsom-stm32h757-tester
ProjectManager.ProjectStructure=M7\:CortexM7 Project\:true;M4\:CortexM4 Project\:true;
ProjectManager.RegisterCallBack=FDCAN,I2S,LPTIM,UART
ProjectManager.StackSize=M4-0x400,M7-0x400
ProjectManager.TargetToolchain=STM32CubeIDE
ProjectManager.ToolChainLocation=
ProjectManager.UAScriptAfterPath=
ProjectManager.UAScriptBeforePath=
ProjectManager.UnderRoot=true
ProjectManager.functionlistsort=1-SystemClock_Config-RCC-false-HAL-false-CortexM7,2-MX_GPIO_Init-GPIO-false-HAL-true-CortexM7,3-MX_DMA_Init-DMA-false-HAL-true-CortexM7,4-MX_FREERTOS_Init-FREERTOS_M7-false-HAL-false-CortexM7,5-MX_USART1_UART_Init-USART1-false-HAL-true-CortexM7,6-MX_LTDC_Init-LTDC-false-HAL-true-CortexM7,7-MX_FMC_Init-FMC-false-HAL-true-CortexM7,8-MX_DMA2D_Init-DMA2D-false-HAL-true-CortexM7,9-MX_DSIHOST_DSI_Init-DSIHOST-false-HAL-true-CortexM7,10-MX_I2C3_Init-I2C3-false-HAL-true-CortexM7,11-MX_LWIP_Init-LWIP-false-HAL-false-CortexM7,12-MX_USB_HOST_Init-USB_HOST_M7-false-HAL-false-CortexM7,13-MX_DCMI_Init-DCMI-false-HAL-true-CortexM7,14-MX_QUADSPI_Init-QUADSPI-false-HAL-true-CortexM7,15-MX_FDCAN1_Init-FDCAN1-false-HAL-true-CortexM7,16-MX_USART6_UART_Init-USART6-false-HAL-true-CortexM7,17-MX_I2C1_Init-I2C1-false-HAL-true-CortexM7,18-MX_I2S2_Init-I2S2-false-HAL-true-CortexM7,19-MX_USART2_UART_Init-USART2-false-HAL-true-CortexM7,20-MX_LPTIM1_Init-LPTIM1-false-HAL-true-CortexM7,21-MX_SDMMC1_SD_Init-SDMMC1-false-HAL-true-CortexM7,22-MX_FATFS_Init-FATFS_M7-false-HAL-false-CortexM7,23-MX_ADC3_Init-ADC3-false-HAL-true-CortexM7,24-MX_ADC1_Init-ADC1-false-HAL-true-CortexM7,1-MX_DMA_Init-DMA-false-HAL-true-CortexM4,0-MX_CORTEX_M7_Init-CORTEX_M7-false-HAL-true-CortexM7,0-MX_CORTEX_M4_Init-CORTEX_M4-false-HAL-true-CortexM4
QUADSPI.ChipSelectHighTime=QSPI_CS_HIGH_TIME_3_CYCLE
QUADSPI.ClockPrescaler=1
QUADSPI.DeviceType=SPI_DEVICE_FLASH
QUADSPI.FlashSize=23
QUADSPI.IPParameters=ClockPrescaler,SampleShifting,FlashSize,DeviceType,ChipSelectHighTime
QUADSPI.SampleShifting=QSPI_SAMPLE_SHIFTING_HALFCYCLE
RCC.ADCCLockSelection=RCC_ADCCLKSOURCE_PLL3
RCC.ADCFreq_Value=48437500
RCC.AHB12Freq_Value=200000000
RCC.AHB4Freq_Value=200000000
RCC.APB1Freq_Value=100000000
RCC.APB2Freq_Value=100000000
RCC.APB3Freq_Value=100000000
RCC.APB4Freq_Value=100000000
RCC.AXIClockFreq_Value=200000000
RCC.CECFreq_Value=32000
RCC.CKPERFreq_Value=64000000
RCC.CPU2Freq_Value=200000000
RCC.CPU2SystikFreq_Value=200000000
RCC.CortexFreq_Value=400000000
RCC.CpuClockFreq_Value=400000000
RCC.D1CPREFreq_Value=400000000
RCC.D1PPRE=RCC_APB3_DIV2
RCC.D2PPRE1=RCC_APB1_DIV2
RCC.D2PPRE2=RCC_APB2_DIV2
RCC.D3PPRE=RCC_APB4_DIV2
RCC.DFSDMACLkFreq_Value=200000000
RCC.DFSDMFreq_Value=100000000
RCC.DIVM1=5
RCC.DIVM2=2
RCC.DIVM3=10
RCC.DIVN1=160
RCC.DIVN2=64
RCC.DIVN3=155
RCC.DIVP1Freq_Value=400000000
RCC.DIVP2Freq_Value=400000000
RCC.DIVP3Freq_Value=193750000
RCC.DIVQ1=4
RCC.DIVQ1Freq_Value=200000000
RCC.DIVQ2=10
RCC.DIVQ2Freq_Value=80000000
RCC.DIVQ3Freq_Value=193750000
RCC.DIVR1Freq_Value=400000000
RCC.DIVR2=13
RCC.DIVR2Freq_Value=61538461.538461536
RCC.DIVR3=8
RCC.DIVR3Freq_Value=48437500
RCC.DSIFreq_Value=61979166.666666664
RCC.DSITXEscFreq_Value=15494791.666666666
RCC.FDCANCLockSelection=RCC_FDCANCLKSOURCE_PLL2
RCC.FDCANFreq_Value=80000000
RCC.FMCFreq_Value=200000000
RCC.FamilyName=M
RCC.HCLK3ClockFreq_Value=200000000
RCC.HCLKFreq_Value=200000000
RCC.HPRE=RCC_HCLK_DIV2
RCC.HRTIMFreq_Value=200000000
RCC.I2C123Freq_Value=100000000
RCC.I2C4Freq_Value=100000000
RCC.IPParameters=ADCCLockSelection,ADCFreq_Value,AHB12Freq_Value,AHB4Freq_Value,APB1Freq_Value,APB2Freq_Value,APB3Freq_Value,APB4Freq_Value,AXIClockFreq_Value,CECFreq_Value,CKPERFreq_Value,CPU2Freq_Value,CPU2SystikFreq_Value,CortexFreq_Value,CpuClockFreq_Value,D1CPREFreq_Value,D1PPRE,D2PPRE1,D2PPRE2,D3PPRE,DFSDMACLkFreq_Value,DFSDMFreq_Value,DIVM1,DIVM2,DIVM3,DIVN1,DIVN2,DIVN3,DIVP1Freq_Value,DIVP2Freq_Value,DIVP3Freq_Value,DIVQ1,DIVQ1Freq_Value,DIVQ2,DIVQ2Freq_Value,DIVQ3Freq_Value,DIVR1Freq_Value,DIVR2,DIVR2Freq_Value,DIVR3,DIVR3Freq_Value,DSIFreq_Value,DSITXEscFreq_Value,FDCANCLockSelection,FDCANFreq_Value,FMCFreq_Value,FamilyName,HCLK3ClockFreq_Value,HCLKFreq_Value,HPRE,HRTIMFreq_Value,I2C123Freq_Value,I2C4Freq_Value,LPTIM1CLockSelection,LPTIM1Freq_Value,LPTIM2Freq_Value,LPTIM345Freq_Value,LPUART1Freq_Value,LTDCFreq_Value,MCO1PinFreq_Value,MCO2PinFreq_Value,PLL1_VCI_Range-AdvancedSettings,PLL1_VCO_SEL-AdvancedSettings,PLL2_VCI_Range-AdvancedSettings,PLL2_VCO_SEL-AdvancedSettings,PLLDSIFreq_Value,PLLDSIIDF,PLLDSINDIV,PLLDSIODF,PLLDSIVCOFreq_Value,PLLSourceVirtual,PWR_Regulator_Voltage_Scale,QSPIFreq_Value,RCC_MCO1Source,RNGFreq_Value,RTCFreq_Value,SAI1Freq_Value,SAI23Freq_Value,SAI4AFreq_Value,SAI4BFreq_Value,SDMMC1CLockSelection,SDMMCFreq_Value,SPDIFRXFreq_Value,SPI123Freq_Value,SPI45Freq_Value,SPI6Freq_Value,SWPMI1Freq_Value,SYSCLKFreq_VALUE,SYSCLKSource,Tim1OutputFreq_Value,Tim2OutputFreq_Value,TraceFreq_Value,USART16Freq_Value,USART234578Freq_Value,USBCLockSelection,USBFreq_Value,VCO1OutputFreq_Value,VCO2OutputFreq_Value,VCO3OutputFreq_Value,VCOInput1Freq_Value,VCOInput2Freq_Value,VCOInput3Freq_Value
RCC.LPTIM1CLockSelection=RCC_LPTIM1CLKSOURCE_LSE
RCC.LPTIM1Freq_Value=32768
RCC.LPTIM2Freq_Value=100000000
RCC.LPTIM345Freq_Value=100000000
RCC.LPUART1Freq_Value=100000000
RCC.LTDCFreq_Value=48437500
RCC.MCO1PinFreq_Value=25000000
RCC.MCO2PinFreq_Value=400000000
RCC.PLL1_VCI_Range-AdvancedSettings=RCC_PLL1VCIRANGE_0
RCC.PLL1_VCO_SEL-AdvancedSettings=RCC_PLL1VCOMEDIUM
RCC.PLL2_VCI_Range-AdvancedSettings=RCC_PLL2VCIRANGE_0
RCC.PLL2_VCO_SEL-AdvancedSettings=RCC_PLL2VCOMEDIUM
RCC.PLLDSIFreq_Value=495833333.3333333
RCC.PLLDSIIDF=DSI_PLL_IN_DIV3
RCC.PLLDSINDIV=119
RCC.PLLDSIODF=DSI_PLL_OUT_DIV2
RCC.PLLDSIVCOFreq_Value=1983333333.3333333
RCC.PLLSourceVirtual=RCC_PLLSOURCE_HSE
RCC.PWR_Regulator_Voltage_Scale=PWR_REGULATOR_VOLTAGE_SCALE1
RCC.QSPIFreq_Value=200000000
RCC.RCC_MCO1Source=RCC_MCO1SOURCE_HSE
RCC.RNGFreq_Value=48000000
RCC.RTCFreq_Value=32000
RCC.SAI1Freq_Value=200000000
RCC.SAI23Freq_Value=200000000
RCC.SAI4AFreq_Value=200000000
RCC.SAI4BFreq_Value=200000000
RCC.SDMMC1CLockSelection=RCC_SDMMCCLKSOURCE_PLL2
RCC.SDMMCFreq_Value=61538461.538461536
RCC.SPDIFRXFreq_Value=200000000
RCC.SPI123Freq_Value=200000000
RCC.SPI45Freq_Value=100000000
RCC.SPI6Freq_Value=100000000
RCC.SWPMI1Freq_Value=100000000
RCC.SYSCLKFreq_VALUE=400000000
RCC.SYSCLKSource=RCC_SYSCLKSOURCE_PLLCLK
RCC.Tim1OutputFreq_Value=200000000
RCC.Tim2OutputFreq_Value=200000000
RCC.TraceFreq_Value=64000000
RCC.USART16Freq_Value=100000000
RCC.USART234578Freq_Value=100000000
RCC.USBCLockSelection=RCC_USBCLKSOURCE_HSI48
RCC.USBFreq_Value=48000000
RCC.VCO1OutputFreq_Value=800000000
RCC.VCO2OutputFreq_Value=800000000
RCC.VCO3OutputFreq_Value=387500000
RCC.VCOInput1Freq_Value=5000000
RCC.VCOInput2Freq_Value=12500000
RCC.VCOInput3Freq_Value=2500000
SH.ADCx_INP0.0=ADC1_INP0,IN0-Single-Ended
SH.ADCx_INP0.ConfNb=1
SH.ADCx_INP1.0=ADC1_INP1,IN1-Single-Ended
SH.ADCx_INP1.ConfNb=1
SH.FMC_A0.0=FMC_A0,13b-sda1
SH.FMC_A0.ConfNb=1
SH.FMC_A1.0=FMC_A1,13b-sda1
SH.FMC_A1.ConfNb=1
SH.FMC_A10.0=FMC_A10,13b-sda1
SH.FMC_A10.ConfNb=1
SH.FMC_A11.0=FMC_A11,13b-sda1
SH.FMC_A11.ConfNb=1
SH.FMC_A12.0=FMC_A12,13b-sda1
SH.FMC_A12.ConfNb=1
SH.FMC_A14_BA0.0=FMC_BA0,FourSdramBanks1
SH.FMC_A14_BA0.ConfNb=1
SH.FMC_A15_BA1.0=FMC_BA1,FourSdramBanks1
SH.FMC_A15_BA1.ConfNb=1
SH.FMC_A2.0=FMC_A2,13b-sda1
SH.FMC_A2.ConfNb=1
SH.FMC_A3.0=FMC_A3,13b-sda1
SH.FMC_A3.ConfNb=1
SH.FMC_A4.0=FMC_A4,13b-sda1
SH.FMC_A4.ConfNb=1
SH.FMC_A5.0=FMC_A5,13b-sda1
SH.FMC_A5.ConfNb=1
SH.FMC_A6.0=FMC_A6,13b-sda1
SH.FMC_A6.ConfNb=1
SH.FMC_A7.0=FMC_A7,13b-sda1
SH.FMC_A7.ConfNb=1
SH.FMC_A8.0=FMC_A8,13b-sda1
SH.FMC_A8.ConfNb=1
SH.FMC_A9.0=FMC_A9,13b-sda1
SH.FMC_A9.ConfNb=1
SH.FMC_D0_DA0.0=FMC_D0,sd-16b-d1
SH.FMC_D0_DA0.ConfNb=1
SH.FMC_D10_DA10.0=FMC_D10,sd-16b-d1
SH.FMC_D10_DA10.ConfNb=1
SH.FMC_D11_DA11.0=FMC_D11,sd-16b-d1
SH.FMC_D11_DA11.ConfNb=1
SH.FMC_D12_DA12.0=FMC_D12,sd-16b-d1
SH.FMC_D12_DA12.ConfNb=1
SH.FMC_D13_DA13.0=FMC_D13,sd-16b-d1
SH.FMC_D13_DA13.ConfNb=1
SH.FMC_D14_DA14.0=FMC_D14,sd-16b-d1
SH.FMC_D14_DA14.ConfNb=1
SH.FMC_D15_DA15.0=FMC_D15,sd-16b-d1
SH.FMC_D15_DA15.ConfNb=1
SH.FMC_D1_DA1.0=FMC_D1,sd-16b-d1
SH.FMC_D1_DA1.ConfNb=1
SH.FMC_D2_DA2.0=FMC_D2,sd-16b-d1
SH.FMC_D2_DA2.ConfNb=1
SH.FMC_D3_DA3.0=FMC_D3,sd-16b-d1
SH.FMC_D3_DA3.ConfNb=1
SH.FMC_D4_DA4.0=FMC_D4,sd-16b-d1
SH.FMC_D4_DA4.ConfNb=1
SH.FMC_D5_DA5.0=FMC_D5,sd-16b-d1
SH.FMC_D5_DA5.ConfNb=1
SH.FMC_D6_DA6.0=FMC_D6,sd-16b-d1
SH.FMC_D6_DA6.ConfNb=1
SH.FMC_D7_DA7.0=FMC_D7,sd-16b-d1
SH.FMC_D7_DA7.ConfNb=1
SH.FMC_D8_DA8.0=FMC_D8,sd-16b-d1
SH.FMC_D8_DA8.ConfNb=1
SH.FMC_D9_DA9.0=FMC_D9,sd-16b-d1
SH.FMC_D9_DA9.ConfNb=1
SH.FMC_NBL0.0=FMC_NBL0,Sd2ByteEnable1
SH.FMC_NBL0.ConfNb=1
SH.FMC_NBL1.0=FMC_NBL1,Sd2ByteEnable1
SH.FMC_NBL1.ConfNb=1
SH.FMC_SDCLK.0=FMC_SDCLK,13b-sda1
SH.FMC_SDCLK.ConfNb=1
SH.FMC_SDNCAS.0=FMC_SDNCAS,13b-sda1
SH.FMC_SDNCAS.ConfNb=1
SH.FMC_SDNRAS.0=FMC_SDNRAS,13b-sda1
SH.FMC_SDNRAS.ConfNb=1
SH.FMC_SDNWE.0=FMC_SDNWE,13b-sda1
SH.FMC_SDNWE.ConfNb=1
SH.GPXTI10.0=GPIO_EXTI10
SH.GPXTI10.ConfNb=1
SH.GPXTI3.0=GPIO_EXTI3
SH.GPXTI3.ConfNb=1
SYS.userName=SYS_M7
USART1.IPParameters=VirtualMode-Asynchronous
USART1.VirtualMode-Asynchronous=VM_ASYNC
USART2.IPParameters=VirtualMode-Asynchronous
USART2.VirtualMode-Asynchronous=VM_ASYNC
USART6.BaudRate=9600
USART6.IPParameters=VirtualMode-Asynchronous,BaudRate
USART6.VirtualMode-Asynchronous=VM_ASYNC
USB_HOST.BSP.number=2
USB_HOST0.BSP.STBoard=false
USB_HOST0.BSP.api=Unknown
USB_HOST0.BSP.component=
USB_HOST0.BSP.condition=SW_VBUS_DRIVE_MSC_FS \= false
USB_HOST0.BSP.instance=PB2
USB_HOST0.BSP.ip=GPIO
USB_HOST0.BSP.mode=Output
USB_HOST0.BSP.name=Drive_VBUS_FS
USB_HOST0.BSP.semaphore=
USB_HOST0.BSP.solution=PB2
USB_HOST1.BSP.STBoard=false
USB_HOST1.BSP.api=Unknown
USB_HOST1.BSP.component=
USB_HOST1.BSP.condition=SW_VBUS_DRIVE_MSC_HS \= false
USB_HOST1.BSP.instance=PB1
USB_HOST1.BSP.ip=GPIO
USB_HOST1.BSP.mode=Output
USB_HOST1.BSP.name=Drive_VBUS_HS
USB_HOST1.BSP.semaphore=
USB_HOST1.BSP.solution=PB1
USB_HOST_M7.IPParameters=USBH_HandleTypeDef-MSC_HS,VirtualModeHS,USBH_DEBUG_LEVEL-MSC_HS,USBH_HandleTypeDef-MSC_FS,VirtualModeFS
USB_HOST_M7.USBH_DEBUG_LEVEL-MSC_HS=3
USB_HOST_M7.USBH_HandleTypeDef-MSC_FS=hUsbHostFS
USB_HOST_M7.USBH_HandleTypeDef-MSC_HS=hUsbHostHS
USB_HOST_M7.VirtualModeFS=Msc
USB_HOST_M7.VirtualModeHS=Msc
USB_OTG_FS.IPParameters=VirtualMode,phy_itface
USB_OTG_FS.VirtualMode=Host_Only
USB_OTG_FS.phy_itface=HCD_PHY_EMBEDDED
USB_OTG_HS.IPParameters=VirtualMode-Host_FS
USB_OTG_HS.VirtualMode-Host_FS=Host_FS
VP_DMA2D_VS_DMA2D.Mode=DMA2D_Activate
VP_DMA2D_VS_DMA2D.Signal=DMA2D_VS_DMA2D
VP_FATFS_M7_VS_SDIO.Mode=SDIO
VP_FATFS_M7_VS_SDIO.Signal=FATFS_M7_VS_SDIO
VP_FREERTOS_M7_VS_CMSIS_V2.Mode=CMSIS_V2
VP_FREERTOS_M7_VS_CMSIS_V2.Signal=FREERTOS_M7_VS_CMSIS_V2
VP_LPTIM1_VS_LPTIM_counterModeInternalClock.Mode=Counts__internal_clock_event_00
VP_LPTIM1_VS_LPTIM_counterModeInternalClock.Signal=LPTIM1_VS_LPTIM_counterModeInternalClock
VP_LTDC_DSIMode.Mode=RGB888
VP_LTDC_DSIMode.Signal=LTDC_DSIMode
VP_LWIP_VS_Enabled.Mode=Enabled
VP_LWIP_VS_Enabled.Signal=LWIP_VS_Enabled
VP_MEMORYMAP_VS_MEMORYMAP.Mode=CurAppReg
VP_MEMORYMAP_VS_MEMORYMAP.Signal=MEMORYMAP_VS_MEMORYMAP
VP_SYS_M4_VS_Systick.Mode=SysTick
VP_SYS_M4_VS_Systick.Signal=SYS_M4_VS_Systick
VP_SYS_VS_tim15.Mode=TIM15
VP_SYS_VS_tim15.Signal=SYS_VS_tim15
VP_USB_HOST_M7_VS_USB_HOST_MSC_FS.Mode=MSC_FS
VP_USB_HOST_M7_VS_USB_HOST_MSC_FS.Signal=USB_HOST_M7_VS_USB_HOST_MSC_FS
VP_USB_HOST_M7_VS_USB_HOST_MSC_HS.Mode=MSC_HS
VP_USB_HOST_M7_VS_USB_HOST_MSC_HS.Signal=USB_HOST_M7_VS_USB_HOST_MSC_HS
board=custom
rtos.0.ip=FREERTOS_M7
isbadioc=false
